### Program Association Table

PAT Version Number: 1
Transport Stream ID: 9307 (0x245b)
PMT PID 48 (0x0030) - Program 42.1/1 KUVE-CD
PMT PID 64 (0x0040) - Program 42.2/2 KFTU-HD
PMT PID 80 (0x0050) - Program 42.3/3 GET.tv
PMT PID 96 (0x0060) - Program 42.4/4 MVSGLD
PMT PID 112 (0x0070) - Program 42.5/5 ShopLC
PMT PID 128 (0x0080) - Program 42.6/6 DABL
PMT PID 144 (0x0090) - Program 42.7/7 BT2

### Program Map Table(s)

Program Number: 42.1/1 KUVE-CD
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 16.708 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 256 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 3/2 5 L, C, R, SL, SR
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x81 AC-3 Audio PID 53 (0x0035)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 42.2/2 KFTU-HD
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 16.708 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 256 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 3/2 5 L, C, R, SL, SR
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x81 AC-3 Audio PID 69 (0x0045)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 42.3/3 GET.tv
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 3.896 Mbps Resolution 640 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 42.4/4 MVSGLD
Descriptor: Smoothing Buffer Descriptor
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0061
Stream Type: 0x1b H.264 Video PID 97 (0x0061)
H.264 Video: Resolution 640 x 480 Interlaced: 1
H.264 Video: Framerate: 59.94 Aspect Ratio: Reserved
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 42.5/5 ShopLC
Descriptor: Smoothing Buffer Descriptor
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0071
Stream Type: 0x1b H.264 Video PID 113 (0x0071)
H.264 Video: Resolution 640 x 480 Interlaced: 1
H.264 Video: Framerate: 59.94 Aspect Ratio: Reserved
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 42.6/6 DABL
Descriptor: Smoothing Buffer Descriptor
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0081
Stream Type: 0x02 MPEG-2 Video PID 129 (0x0081)
MPEG Video: Bitrate 3.896 Mbps Resolution 640 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 132 (0x0084)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 42.7/7 BT2
Descriptor: Smoothing Buffer Descriptor
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0091
Stream Type: 0x1b H.264 Video PID 145 (0x0091)
H.264 Video: Resolution 640 x 480 Interlaced: 1
H.264 Video: Framerate: 59.94 Aspect Ratio: Reserved
Stream Type: 0x81 AC-3 Audio PID 148 (0x0094)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: KUVE-CD
TSID: 9307 (0x245b)
Channel Number: 42.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = spa
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0035 Language = mul

Channel 2
Service Name: KFTU-HD
TSID: 9307 (0x245b)
Channel Number: 42.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = spa
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0045 Language = mul

Channel 3
Service Name: GET.tv
TSID: 9307 (0x245b)
Channel Number: 42.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 4
Service Name: MVSGLD
TSID: 9307 (0x245b)
Channel Number: 42.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 5
Service Name: ShopLC
TSID: 9307 (0x245b)
Channel Number: 42.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng
Stream Type 0x1b (H.264 Video) ESPID = 0x0071 Language =

Channel 6
Service Name: DABL
TSID: 9307 (0x245b)
Channel Number: 42.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0081
Stream Type 0x1b (H.264 Video) ESPID = 0x0081 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0084 Language = eng

Channel 7
Service Name: BT2
TSID: 9307 (0x245b)
Channel Number: 42.7
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 0
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0091
Stream Type 0x1b (H.264 Video) ESPID = 0x0091 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0094 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 346 | 0
CAT | 0 | 0
PMT | 14 | 0
ETT | 717 | 0
PSIP | 900 | 0
EIT | 1.2k | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,657 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 36 (605 MHz)
Signal: Locked Signal 69 Quality 90
Network Type: ATSC
Run Time: 000:01:05

### PID Usage Chart

0x0000 (0.04% ~ 0.01 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.04% ~ 0.01 Mbps) |  | 0x0030 MPEG-2 PMT for program 42.1/1
0x0031 (29.75% - 5.78 Mbps) |  | 0x0031 MPEG-2 Video for program 42.1/1
0x0034 (1.37% ~ 0.27 Mbps) |  | 0x0034 AC-3 Audio for program 42.1/1
0x0035 (0.69% ~ 0.13 Mbps) |  | 0x0035 AC-3 Audio for program 42.1/1
0x0040 (0.04% ~ 0.01 Mbps) |  | 0x0040 MPEG-2 PMT for program 42.2/2
0x0041 (33.75% - 6.55 Mbps) |  | 0x0041 MPEG-2 Video for program 42.2/2
0x0044 (1.37% ~ 0.27 Mbps) |  | 0x0044 AC-3 Audio for program 42.2/2
0x0045 (0.69% ~ 0.13 Mbps) |  | 0x0045 AC-3 Audio for program 42.2/2
0x0050 (0.04% ~ 0.01 Mbps) |  | 0x0050 MPEG-2 PMT for program 42.3/3
0x0051 (6.41% - 1.25 Mbps) |  | 0x0051 MPEG-2 Video for program 42.3/3
0x0054 (0.69% ~ 0.13 Mbps) |  | 0x0054 AC-3 Audio for program 42.3/3
0x0060 (0.04% ~ 0.01 Mbps) |  | 0x0060 MPEG-2 PMT for program 42.4/4
0x0061 (2.36% - 0.46 Mbps) |  | 0x0061 H.264 Video for program 42.4/4
0x0064 (0.69% ~ 0.13 Mbps) |  | 0x0064 AC-3 Audio for program 42.4/4
0x0070 (0.04% ~ 0.01 Mbps) |  | 0x0070 MPEG-2 PMT for program 42.5/5
0x0071 (5.17% - 1.00 Mbps) |  | 0x0071 H.264 Video for program 42.5/5
0x0074 (0.69% ~ 0.13 Mbps) |  | 0x0074 AC-3 Audio for program 42.5/5
0x0080 (0.04% ~ 0.01 Mbps) |  | 0x0080 MPEG-2 PMT for program 42.6/6
0x0081 (6.31% - 1.22 Mbps) |  | 0x0081 MPEG-2 Video for program 42.6/6
0x0084 (0.69% ~ 0.13 Mbps) |  | 0x0084 AC-3 Audio for program 42.6/6
0x0090 (0.04% ~ 0.01 Mbps) |  | 0x0090 MPEG-2 PMT for program 42.7/7
0x0091 (4.41% - 0.86 Mbps) |  | 0x0091 H.264 Video for program 42.7/7
0x0094 (0.69% ~ 0.13 Mbps) |  | 0x0094 AC-3 Audio for program 42.7/7
0x1d00 (0.22% ~ 0.04 Mbps) |  | 0x1d00 ATSC EIT-0
0x1d01 (0.03% ~ 0.01 Mbps) |  | 0x1d01 ATSC EIT-1
0x1d02 (0.02% ~ 0.00 Mbps) |  | 0x1d02 ATSC EIT-2
0x1d03 (0.02% ~ 0.00 Mbps) |  | 0x1d03 ATSC EIT-3
0x1e00 (0.03% ~ 0.01 Mbps) |  | 0x1e00 ATSC Event ETT-0
0x1e01 (0.02% ~ 0.00 Mbps) |  | 0x1e01 ATSC Event ETT-1
0x1e02 (0.02% ~ 0.00 Mbps) |  | 0x1e02 ATSC Event ETT-2
0x1e03 (0.03% ~ 0.00 Mbps) |  | 0x1e03 ATSC Event ETT-3
0x1ffb (0.15% ~ 0.03 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (3.42% ~ 0.66 Mbps) |  | 0x1fff MPEG-2 NULL Packet