### Program Association Table

PAT Version Number: 0
Transport Stream ID: 219 (0x00db)
PMT PID 48 (0x0030) - Program 13.1/3 KOLD DT
PMT PID 64 (0x0040) - Program 13.2/4 Me TV
PMT PID 80 (0x0050) - Program 13.3/5 AZSPORT
PMT PID 96 (0x0060) - Program 13.4/6 IONPlus
PMT PID 112 (0x0070) - Program 13.5/7 Outlaw
PMT PID 128 (0x0080) - Program 13.6/8 Charge
PMT PID 144 (0x0090) - Program 40.4/9 Oxygen

### Program Map Table(s)

Program Number: 13.1/3 KOLD DT
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 14.172 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 384 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 3/2 5 L, C, R, SL, SR
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Stream Type: 0x81 AC-3 Audio PID 53 (0x0035)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 13.2/4 Me TV
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 4.875 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 13.3/5 AZSPORT
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 11.717 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 13.4/6 IONPlus
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 4.875 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 13.5/7 Outlaw
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 4.875 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 13.6/8 Charge
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0081
Stream Type: 0x02 MPEG-2 Video PID 129 (0x0081)
MPEG Video: Bitrate 4.875 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 132 (0x0084)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 40.4/9 Oxygen
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0091
Stream Type: 0x02 MPEG-2 Video PID 145 (0x0091)
MPEG Video: Bitrate 4.875 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 148 (0x0094)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

### Terrestrial Virtual Channel Table

Channel 3
Service Name: KOLD DT
TSID: 219 (0x00db) Old-NTSC: 13 ATSC: 32 AZ TUCSON
Channel Number: 13.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0035 Language = spa

Channel 4
Service Name: Me TV
TSID: 219 (0x00db) Old-NTSC: 13 ATSC: 32 AZ TUCSON
Channel Number: 13.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 5
Service Name: AZSPORT
TSID: 219 (0x00db) Old-NTSC: 13 ATSC: 32 AZ TUCSON
Channel Number: 13.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 6
Service Name: IONPlus
TSID: 219 (0x00db) Old-NTSC: 13 ATSC: 32 AZ TUCSON
Channel Number: 13.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 7
Service Name: Outlaw
TSID: 219 (0x00db) Old-NTSC: 13 ATSC: 32 AZ TUCSON
Channel Number: 13.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng

Channel 8
Service Name: Charge
TSID: 219 (0x00db) Old-NTSC: 13 ATSC: 32 AZ TUCSON
Channel Number: 13.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0081
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0081 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0084 Language = eng

Channel 9
Service Name: Oxygen
TSID: 219 (0x00db) Old-NTSC: 13 ATSC: 32 AZ TUCSON
Channel Number: 40.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 7
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0091
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0091 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0094 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 16.9k | 0
CAT | 0 | 0
PMT | 14 | 0
ETT | 190.8k | 2
PSIP | 17.6k | 1
EIT | 56.1k | 0

Continuity errors: 646
TEI errors: 185
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,389,261 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 13 (213 MHz)
Signal: Locked Signal 45 Quality 51
Network Type: ATSC
Run Time: 000:28:12

### PID Usage Chart

0x0000 (0.08% ~ 0.02 Mbps) *3/0 |  | 0x0000 MPEG-2 Program Assocation Table
0x0027 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0027 Unknown usage
0x0030 (0.04% ~ 0.01 Mbps) *3/0 |  | 0x0030 MPEG-2 PMT for program 13.1/3
0x0031 (29.66% - 5.75 Mbps) *39/65 |  | 0x0031 MPEG-2 Video for program 13.1/3
0x0033 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0033 Unknown usage
0x0034 (2.04% ~ 0.39 Mbps) *41/6 |  | 0x0034 AC-3 Audio for program 13.1/3
0x0035 (1.02% ~ 0.20 Mbps) *20/2 |  | 0x0035 AC-3 Audio for program 13.1/3
0x0040 (0.04% ~ 0.01 Mbps) *5/1 |  | 0x0040 MPEG-2 PMT for program 13.2/4
0x0041 (7.15% - 1.39 Mbps) *38/13 |  | 0x0041 MPEG-2 Video for program 13.2/4
0x0043 (0.00% ~ 0.00 Mbps) *1/2 |  | 0x0043 Unknown usage
0x0044 (1.02% ~ 0.20 Mbps) *40/1 |  | 0x0044 AC-3 Audio for program 13.2/4
0x0050 (0.04% ~ 0.01 Mbps) *3/0 |  | 0x0050 MPEG-2 PMT for program 13.3/5
0x0051 (25.02% - 4.86 Mbps) *40/35 |  | 0x0051 MPEG-2 Video for program 13.3/5
0x0054 (1.02% ~ 0.20 Mbps) *38/2 |  | 0x0054 AC-3 Audio for program 13.3/5
0x0060 (0.04% ~ 0.01 Mbps) *3/0 |  | 0x0060 MPEG-2 PMT for program 13.4/6
0x0061 (6.19% - 1.20 Mbps) *42/8 |  | 0x0061 MPEG-2 Video for program 13.4/6
0x0064 (1.02% ~ 0.20 Mbps) *38/2 |  | 0x0064 AC-3 Audio for program 13.4/6
0x0070 (0.04% ~ 0.01 Mbps) *3/0 |  | 0x0070 MPEG-2 PMT for program 13.5/7
0x0071 (5.50% - 1.07 Mbps) *33/7 |  | 0x0071 MPEG-2 Video for program 13.5/7
0x0074 (1.02% ~ 0.20 Mbps) *40/2 |  | 0x0074 AC-3 Audio for program 13.5/7
0x0080 (0.04% ~ 0.01 Mbps) *3/0 |  | 0x0080 MPEG-2 PMT for program 13.6/8
0x0081 (4.84% - 0.94 Mbps) *39/12 |  | 0x0081 MPEG-2 Video for program 13.6/8
0x0084 (1.02% ~ 0.20 Mbps) *38/1 |  | 0x0084 AC-3 Audio for program 13.6/8
0x0090 (0.04% ~ 0.01 Mbps) *5/1 |  | 0x0090 MPEG-2 PMT for program 40.4/9
0x0091 (7.25% - 1.41 Mbps) *34/11 |  | 0x0091 MPEG-2 Video for program 40.4/9
0x0094 (1.02% ~ 0.20 Mbps) *38/1 |  | 0x0094 AC-3 Audio for program 40.4/9
0x00a0 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x00a0 Unknown usage
0x00ad (0.00% ~ 0.00 Mbps) *0/1 |  | 0x00ad Unknown usage
0x00c9 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x00c9 Unknown usage
0x00d1 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x00d1 Unknown usage
0x1d00 (0.25% ~ 0.05 Mbps) *4/0 |  | 0x1d00 ATSC EIT-0
0x1d01 (0.08% ~ 0.02 Mbps) *1/0 |  | 0x1d01 ATSC EIT-1
0x1d02 (0.04% ~ 0.01 Mbps) *1/0 |  | 0x1d02 ATSC EIT-2
0x1d03 (0.03% ~ 0.01 Mbps) *2/0 |  | 0x1d03 ATSC EIT-3
0x1d04 (0.02% ~ 0.00 Mbps) *2/0 |  | 0x1d04 ATSC EIT-4
0x1d05 (0.02% ~ 0.00 Mbps) *2/0 |  | 0x1d05 ATSC EIT-5
0x1d06 (0.02% ~ 0.00 Mbps) *3/0 |  | 0x1d06 ATSC EIT-6
0x1d07 (0.01% ~ 0.00 Mbps) |  | 0x1d07 ATSC EIT-7
0x1d08 (0.01% ~ 0.00 Mbps) |  | 0x1d08 ATSC EIT-8
0x1d09 (0.01% ~ 0.00 Mbps) |  | 0x1d09 ATSC EIT-9
0x1d0a (0.01% ~ 0.00 Mbps) |  | 0x1d0a ATSC EIT-10
0x1d0b (0.01% ~ 0.00 Mbps) |  | 0x1d0b ATSC EIT-11
0x1d0c (0.01% ~ 0.00 Mbps) |  | 0x1d0c ATSC EIT-12
0x1d0d (0.01% ~ 0.00 Mbps) |  | 0x1d0d ATSC EIT-13
0x1d0e (0.01% ~ 0.00 Mbps) |  | 0x1d0e ATSC EIT-14
0x1d0f (0.01% ~ 0.00 Mbps) |  | 0x1d0f ATSC EIT-15
0x1e00 (0.73% ~ 0.14 Mbps) *20/2 |  | 0x1e00 ATSC Event ETT-0
0x1e01 (0.23% ~ 0.04 Mbps) *5/0 |  | 0x1e01 ATSC Event ETT-1
0x1e02 (0.11% ~ 0.02 Mbps) *3/0 |  | 0x1e02 ATSC Event ETT-2
0x1e03 (0.08% ~ 0.02 Mbps) *2/0 |  | 0x1e03 ATSC Event ETT-3
0x1e04 (0.07% ~ 0.01 Mbps) *2/0 |  | 0x1e04 ATSC Event ETT-4
0x1e05 (0.05% ~ 0.01 Mbps) *1/0 |  | 0x1e05 ATSC Event ETT-5
0x1e06 (0.05% ~ 0.01 Mbps) *1/0 |  | 0x1e06 ATSC Event ETT-6
0x1e07 (0.04% ~ 0.01 Mbps) |  | 0x1e07 ATSC Event ETT-7
0x1e08 (0.03% ~ 0.01 Mbps) |  | 0x1e08 ATSC Event ETT-8
0x1e09 (0.02% ~ 0.00 Mbps) *2/0 |  | 0x1e09 ATSC Event ETT-9
0x1e0a (0.03% ~ 0.01 Mbps) *2/0 |  | 0x1e0a ATSC Event ETT-10
0x1e0b (0.03% ~ 0.00 Mbps) *3/0 |  | 0x1e0b ATSC Event ETT-11
0x1e0c (0.03% ~ 0.00 Mbps) |  | 0x1e0c ATSC Event ETT-12
0x1e0d (0.02% ~ 0.00 Mbps) |  | 0x1e0d ATSC Event ETT-13
0x1e0e (0.02% ~ 0.00 Mbps) *1/0 |  | 0x1e0e ATSC Event ETT-14
0x1e0f (0.02% ~ 0.00 Mbps) |  | 0x1e0f ATSC Event ETT-15
0x1ffb (0.20% ~ 0.04 Mbps) *2/1 |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (2.59% ~ 0.50 Mbps) *0/4 |  | 0x1fff MPEG-2 NULL Packet