### Program Association Table

PAT Version Number: 30
Transport Stream ID: 2415 (0x096f)
PMT PID 48 (0x0030) - Program 12.1/1 KDRV-HD
PMT PID 64 (0x0040) - Program 12.2/2 KDRVDT2
PMT PID 80 (0x0050) - Program 12.3/3 KDRVDT3
PMT PID 96 (0x0060) - Program 12.4/4 KDRVDT4
PMT PID 112 (0x0070) - Program 12.5/5 KDRVDT5

### Program Map Table(s)

Program Number: 12.1/1 KDRV-HD
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 0.951 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 384 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 3/2 5 L, C, R, SL, SR
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x81 AC-3 Audio PID 53 (0x0035)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode visually impaired Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 12.2/2 KDRVDT2
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 0.275 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 12.3/3 KDRVDT3
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 0.275 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 12.4/4 KDRVDT4
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 2.917 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 12.5/5 KDRVDT5
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 2.917 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: KDRV-HD
TSID: 2415 (0x096f) VCh: 12 RFCh: 12 KDRV MEDFORD, OR
Channel Number: 12.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0035 Language = spa

Channel 2
Service Name: KDRVDT2
TSID: 2415 (0x096f) VCh: 12 RFCh: 12 KDRV MEDFORD, OR
Channel Number: 12.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 3
Service Name: KDRVDT3
TSID: 2415 (0x096f) VCh: 12 RFCh: 12 KDRV MEDFORD, OR
Channel Number: 12.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 4
Service Name: KDRVDT4
TSID: 2415 (0x096f) VCh: 12 RFCh: 12 KDRV MEDFORD, OR
Channel Number: 12.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 5
Service Name: KDRVDT5
TSID: 2415 (0x096f) VCh: 12 RFCh: 12 KDRV MEDFORD, OR
Channel Number: 12.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 1.0k | 0
CAT | 0 | 0
PMT | 10 | 0
ETT | 178 | 0
PSIP | 1.1k | 0
EIT | 1.7k | 0

Continuity errors: 0
TEI errors: 49
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,731 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 21 (515 MHz)
Signal: Locked Signal 68 Quality 71
Network Type: ATSC
Run Time: 000:01:38

### PID Usage Chart

0x0000 (0.08% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.08% ~ 0.02 Mbps) |  | 0x0030 MPEG-2 PMT for program 12.1/1
0x0031 (45.93% - 8.91 Mbps) *0/31 |  | 0x0031 MPEG-2 Video for program 12.1/1
0x0034 (2.06% ~ 0.40 Mbps) |  | 0x0034 AC-3 Audio for program 12.1/1
0x0035 (1.05% ~ 0.20 Mbps) *0/1 |  | 0x0035 AC-3 Audio for program 12.1/1
0x0040 (0.08% ~ 0.02 Mbps) |  | 0x0040 MPEG-2 PMT for program 12.2/2
0x0041 (10.24% - 1.99 Mbps) *0/2 |  | 0x0041 MPEG-2 Video for program 12.2/2
0x0044 (1.05% ~ 0.20 Mbps) |  | 0x0044 AC-3 Audio for program 12.2/2
0x0050 (0.08% ~ 0.02 Mbps) |  | 0x0050 MPEG-2 PMT for program 12.3/3
0x0051 (9.17% - 1.78 Mbps) *0/2 |  | 0x0051 MPEG-2 Video for program 12.3/3
0x0054 (1.05% ~ 0.20 Mbps) *0/1 |  | 0x0054 AC-3 Audio for program 12.3/3
0x0060 (0.08% ~ 0.02 Mbps) |  | 0x0060 MPEG-2 PMT for program 12.4/4
0x0061 (11.96% - 2.32 Mbps) *0/4 |  | 0x0061 MPEG-2 Video for program 12.4/4
0x0064 (1.05% ~ 0.20 Mbps) *0/1 |  | 0x0064 AC-3 Audio for program 12.4/4
0x0070 (0.08% ~ 0.02 Mbps) |  | 0x0070 MPEG-2 PMT for program 12.5/5
0x0071 (11.77% - 2.28 Mbps) *0/5 |  | 0x0071 MPEG-2 Video for program 12.5/5
0x0074 (1.05% ~ 0.20 Mbps) *0/1 |  | 0x0074 AC-3 Audio for program 12.5/5
0x1388 (0.02% ~ 0.00 Mbps) |  | 0x1388 ATSC EIT-3
0x1389 (0.13% ~ 0.02 Mbps) |  | 0x1389 ATSC EIT-0
0x138a (0.04% ~ 0.01 Mbps) |  | 0x138a ATSC EIT-1
0x138b (0.03% ~ 0.01 Mbps) |  | 0x138b ATSC EIT-2
0x13ec (0.00% ~ 0.00 Mbps) |  | 0x13ec ATSC Event ETT-3
0x13ed (0.00% ~ 0.00 Mbps) |  | 0x13ed ATSC Event ETT-0
0x13ee (0.00% ~ 0.00 Mbps) |  | 0x13ee ATSC Event ETT-1
0x13ef (0.00% ~ 0.00 Mbps) |  | 0x13ef ATSC Event ETT-2
0x1ffb (0.10% ~ 0.02 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (2.81% ~ 0.55 Mbps) *0/1 |  | 0x1fff MPEG-2 NULL Packet