### Program Association Table

PAT Version Number: 0
Transport Stream ID: 2089 (0x0829)
PMT PID 48 (0x0030) - Program 3.1/3 NBC3
PMT PID 64 (0x0040) - Program 3.2/4 ROAR
PMT PID 80 (0x0050) - Program 3.3/5 Charge!
PMT PID 96 (0x0060) - Program 3.4/6 Comet
PMT PID 112 (0x0070) - Program 33.2/7 My_LVTV

### Program Map Table(s)

Program Number: 3.1/3 NBC3
Descriptor: Registration Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 14.368 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 384 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 3/2 5 L, C, R, SL, SR
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Stream Type: 0x81 AC-3 Audio PID 53 (0x0035)
AC3: Bitrate 96 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 1/0 C
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 3.2/4 ROAR
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 9.674 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 3.3/5 Charge!
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 5.674 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 3.4/6 Comet
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 5.674 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 33.2/7 My_LVTV
Descriptor: Registration Descriptor
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 9.270 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 384 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Stream Type: 0x81 AC-3 Audio PID 117 (0x0075)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

### Terrestrial Virtual Channel Table

Channel 3
Service Name: NBC3
TSID: 2089 (0x0829) VCh: 3 RFCh: 22 KSNV LAS VEGAS, NV
Channel Number: 3.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0035 Language = spa

Channel 4
Service Name: ROAR
TSID: 2089 (0x0829) VCh: 3 RFCh: 22 KSNV LAS VEGAS, NV
Channel Number: 3.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 5
Service Name: Charge!
TSID: 2089 (0x0829) VCh: 3 RFCh: 22 KSNV LAS VEGAS, NV
Channel Number: 3.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 6
Service Name: Comet
TSID: 2089 (0x0829) VCh: 3 RFCh: 22 KSNV LAS VEGAS, NV
Channel Number: 3.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 7
Service Name: My_LVTV
TSID: 2089 (0x0829) VCh: 3 RFCh: 22 KSNV LAS VEGAS, NV
Channel Number: 33.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0075 Language = spa

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 547 | 0
CAT | 0 | 0
PMT | 10 | 0
ETT | 3.2k | 0
PSIP | 501 | 0
EIT | 768 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,657 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 22 (521 MHz)
Signal: Locked Signal 100 Quality 64
Network Type: ATSC
Run Time: 000:00:40

### PID Usage Chart

0x0000 (0.11% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.02% ~ 0.00 Mbps) |  | 0x0030 MPEG-2 PMT for program 3.1/3
0x0031 (36.37% - 7.05 Mbps) |  | 0x0031 MPEG-2 Video for program 3.1/3
0x0034 (2.04% ~ 0.39 Mbps) |  | 0x0034 AC-3 Audio for program 3.1/3
0x0035 (0.53% ~ 0.10 Mbps) |  | 0x0035 AC-3 Audio for program 3.1/3
0x0040 (0.02% ~ 0.00 Mbps) |  | 0x0040 MPEG-2 PMT for program 3.2/4
0x0041 (20.07% - 3.90 Mbps) |  | 0x0041 MPEG-2 Video for program 3.2/4
0x0044 (1.02% ~ 0.20 Mbps) |  | 0x0044 AC-3 Audio for program 3.2/4
0x0050 (0.02% ~ 0.00 Mbps) |  | 0x0050 MPEG-2 PMT for program 3.3/5
0x0051 (9.77% - 1.90 Mbps) |  | 0x0051 MPEG-2 Video for program 3.3/5
0x0054 (1.02% ~ 0.20 Mbps) |  | 0x0054 AC-3 Audio for program 3.3/5
0x0060 (0.02% ~ 0.00 Mbps) |  | 0x0060 MPEG-2 PMT for program 3.4/6
0x0061 (7.51% - 1.46 Mbps) |  | 0x0061 MPEG-2 Video for program 3.4/6
0x0064 (1.02% ~ 0.20 Mbps) |  | 0x0064 AC-3 Audio for program 3.4/6
0x0070 (0.02% ~ 0.00 Mbps) |  | 0x0070 MPEG-2 PMT for program 33.2/7
0x0071 (15.56% - 3.02 Mbps) |  | 0x0071 MPEG-2 Video for program 33.2/7
0x0074 (2.04% ~ 0.39 Mbps) |  | 0x0074 AC-3 Audio for program 33.2/7
0x0075 (1.02% ~ 0.20 Mbps) |  | 0x0075 AC-3 Audio for program 33.2/7
0x1d00 (0.19% ~ 0.04 Mbps) |  | 0x1d00 ATSC EIT-0
0x1d01 (0.06% ~ 0.01 Mbps) |  | 0x1d01 ATSC EIT-1
0x1d02 (0.04% ~ 0.01 Mbps) |  | 0x1d02 ATSC EIT-2
0x1d03 (0.03% ~ 0.00 Mbps) |  | 0x1d03 ATSC EIT-3
0x1e00 (0.58% ~ 0.11 Mbps) |  | 0x1e00 ATSC Event ETT-0
0x1e01 (0.15% ~ 0.03 Mbps) |  | 0x1e01 ATSC Event ETT-1
0x1e02 (0.09% ~ 0.02 Mbps) |  | 0x1e02 ATSC Event ETT-2
0x1e03 (0.05% ~ 0.01 Mbps) |  | 0x1e03 ATSC Event ETT-3
0x1ffb (0.12% ~ 0.02 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (0.51% ~ 0.10 Mbps) |  | 0x1fff MPEG-2 NULL Packet