### Program Association Table

PAT Version Number: 1
Transport Stream ID: 10015 (0x271f)
PMT PID 16 (0x0010) - Network
PMT PID 48 (0x0030) - Program 30.1/1001 KEGS-LD
PMT PID 64 (0x0040) - Program 30.2/1002 KEGS-LD
PMT PID 80 (0x0050) - Program 30.3/1003 KEGS-LD
PMT PID 96 (0x0060) - Program 30.4/1004 KEGS-LD
PMT PID 112 (0x0070) - Program 30.5/1005 KEGS-LD
PMT PID 128 (0x0080) - Program 30.6/1006 KEGS-LD
PMT PID 144 (0x0090) - Program 30.7/1007 KEGS-LD

### Program Map Table(s)

Network PMT Entry - carried on PID 16 (0x0010)

Program Number: 30.1/1001 KEGS-LD
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 1.938 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 30.2/1002 KEGS-LD
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 1.938 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 30.3/1003 KEGS-LD
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 1.848 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 30.4/1004 KEGS-LD
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 2.114 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 30.5/1005 KEGS-LD
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 2.500 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 30.6/1006 KEGS-LD
PCR PID: 0x0081
Stream Type: 0x02 MPEG-2 Video PID 129 (0x0081)
MPEG Video: Bitrate 1.938 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 132 (0x0084)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 30.7/1007 KEGS-LD
PCR PID: 0x0091
Stream Type: 0x02 MPEG-2 Video PID 145 (0x0091)
MPEG Video: Bitrate 1.938 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 148 (0x0094)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

### Terrestrial Virtual Channel Table

Channel 1001
Service Name: KEGS-LD
TSID: 10015 (0x271f)
Channel Number: 30.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng

Channel 1002
Service Name: KEGS-LD
TSID: 10015 (0x271f)
Channel Number: 30.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 1003
Service Name: KEGS-LD
TSID: 10015 (0x271f)
Channel Number: 30.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 1004
Service Name: KEGS-LD
TSID: 10015 (0x271f)
Channel Number: 30.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 1005
Service Name: KEGS-LD
TSID: 10015 (0x271f)
Channel Number: 30.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng

Channel 1006
Service Name: KEGS-LD
TSID: 10015 (0x271f)
Channel Number: 30.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0081
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0081 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0084 Language = eng

Channel 1007
Service Name: KEGS-LD
TSID: 10015 (0x271f)
Channel Number: 30.7
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 7
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0091
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0091 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0094 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 734 | 0
CAT | 0 | 0
PMT | 14 | 0
ETT | 5.3k | 0
PSIP | 2.2k | 0
EIT | 1.5k | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,156 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 24 (533 MHz)
Signal: Locked Signal 79 Quality 52
Network Type: ATSC
Run Time: 000:00:42

### PID Usage Chart

0x0000 (0.14% ~ 0.03 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.14% ~ 0.03 Mbps) |  | 0x0030 MPEG-2 PMT for program 30.1/1001
0x0031 (11.01% - 2.13 Mbps) |  | 0x0031 MPEG-2 Video for program 30.1/1001
0x0034 (1.21% ~ 0.24 Mbps) |  | 0x0034 AC-3 Audio for program 30.1/1001
0x0040 (0.14% ~ 0.03 Mbps) |  | 0x0040 MPEG-2 PMT for program 30.2/1002
0x0041 (11.01% - 2.14 Mbps) |  | 0x0041 MPEG-2 Video for program 30.2/1002
0x0044 (1.21% ~ 0.24 Mbps) |  | 0x0044 AC-3 Audio for program 30.2/1002
0x0050 (0.14% ~ 0.03 Mbps) |  | 0x0050 MPEG-2 PMT for program 30.3/1003
0x0051 (10.51% - 2.04 Mbps) |  | 0x0051 MPEG-2 Video for program 30.3/1003
0x0054 (1.05% ~ 0.20 Mbps) |  | 0x0054 AC-3 Audio for program 30.3/1003
0x0060 (0.14% ~ 0.03 Mbps) |  | 0x0060 MPEG-2 PMT for program 30.4/1004
0x0061 (11.55% - 2.24 Mbps) |  | 0x0061 MPEG-2 Video for program 30.4/1004
0x0064 (1.01% ~ 0.20 Mbps) |  | 0x0064 AC-3 Audio for program 30.4/1004
0x0070 (0.14% ~ 0.03 Mbps) |  | 0x0070 MPEG-2 PMT for program 30.5/1005
0x0071 (11.75% - 2.28 Mbps) |  | 0x0071 MPEG-2 Video for program 30.5/1005
0x0074 (1.01% ~ 0.20 Mbps) |  | 0x0074 AC-3 Audio for program 30.5/1005
0x0080 (0.14% ~ 0.03 Mbps) |  | 0x0080 MPEG-2 PMT for program 30.6/1006
0x0081 (11.01% - 2.13 Mbps) |  | 0x0081 MPEG-2 Video for program 30.6/1006
0x0084 (1.21% ~ 0.24 Mbps) |  | 0x0084 AC-3 Audio for program 30.6/1006
0x0090 (0.14% ~ 0.03 Mbps) |  | 0x0090 MPEG-2 PMT for program 30.7/1007
0x0091 (11.00% - 2.13 Mbps) |  | 0x0091 MPEG-2 Video for program 30.7/1007
0x0094 (1.21% ~ 0.24 Mbps) |  | 0x0094 AC-3 Audio for program 30.7/1007
0x1d00 (0.37% ~ 0.07 Mbps) |  | 0x1d00 ATSC EIT-0
0x1d01 (0.06% ~ 0.01 Mbps) |  | 0x1d01 ATSC EIT-1
0x1d02 (0.01% ~ 0.00 Mbps) |  | 0x1d02 ATSC EIT-2
0x1d03 (0.01% ~ 0.00 Mbps) |  | 0x1d03 ATSC EIT-3
0x1d04 (0.01% ~ 0.00 Mbps) |  | 0x1d04 ATSC EIT-4
0x1d05 (0.01% ~ 0.00 Mbps) |  | 0x1d05 ATSC EIT-5
0x1d06 (0.01% ~ 0.00 Mbps) |  | 0x1d06 ATSC EIT-6
0x1d07 (0.01% ~ 0.00 Mbps) |  | 0x1d07 Unknown usage
0x1d08 (0.01% ~ 0.00 Mbps) |  | 0x1d08 Unknown usage
0x1d09 (0.01% ~ 0.00 Mbps) |  | 0x1d09 Unknown usage
0x1d0a (0.01% ~ 0.00 Mbps) |  | 0x1d0a Unknown usage
0x1d0b (0.01% ~ 0.00 Mbps) |  | 0x1d0b Unknown usage
0x1d0c (0.01% ~ 0.00 Mbps) |  | 0x1d0c Unknown usage
0x1d0d (0.01% ~ 0.00 Mbps) |  | 0x1d0d Unknown usage
0x1d0e (0.01% ~ 0.00 Mbps) |  | 0x1d0e Unknown usage
0x1d0f (0.01% ~ 0.00 Mbps) |  | 0x1d0f Unknown usage
0x1e00 (0.90% ~ 0.18 Mbps) |  | 0x1e00 ATSC Event ETT-0
0x1e01 (0.16% ~ 0.03 Mbps) |  | 0x1e01 ATSC Event ETT-1
0x1e02 (0.01% ~ 0.00 Mbps) |  | 0x1e02 ATSC Event ETT-2
0x1e03 (0.01% ~ 0.00 Mbps) |  | 0x1e03 ATSC Event ETT-3
0x1e04 (0.01% ~ 0.00 Mbps) |  | 0x1e04 ATSC Event ETT-4
0x1e05 (0.01% ~ 0.00 Mbps) |  | 0x1e05 ATSC Event ETT-5
0x1e06 (0.01% ~ 0.00 Mbps) |  | 0x1e06 ATSC Event ETT-6
0x1e07 (0.01% ~ 0.00 Mbps) |  | 0x1e07 Unknown usage
0x1e08 (0.01% ~ 0.00 Mbps) |  | 0x1e08 Unknown usage
0x1e09 (0.01% ~ 0.00 Mbps) |  | 0x1e09 Unknown usage
0x1e0a (0.01% ~ 0.00 Mbps) |  | 0x1e0a Unknown usage
0x1e0b (0.01% ~ 0.00 Mbps) |  | 0x1e0b Unknown usage
0x1e0c (0.01% ~ 0.00 Mbps) |  | 0x1e0c Unknown usage
0x1e0d (0.01% ~ 0.00 Mbps) |  | 0x1e0d Unknown usage
0x1e0e (0.01% ~ 0.00 Mbps) |  | 0x1e0e Unknown usage
0x1e0f (0.01% ~ 0.00 Mbps) |  | 0x1e0f Unknown usage
0x1ffb (0.55% ~ 0.11 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (10.92% ~ 2.12 Mbps) |  | 0x1fff MPEG-2 NULL Packet