### Program Association Table

PAT Version Number: 1
Transport Stream ID: 10851 (0x2a63)
PMT PID 48 (0x0030) - Program 7.1/2 KDNU
PMT PID 64 (0x0040) - Program 7.2/4 Bridge1
PMT PID 80 (0x0050) - Program 7.3/6 InTouch
PMT PID 96 (0x0060) - Program 7.4/8 AWSN
PMT PID 112 (0x0070) - Program 7.5/10 Sales
PMT PID 128 (0x0080) - Program 7.6/12 BarkTV
PMT PID 144 (0x0090) - Program 7.7/14 ZLiving
PMT PID 160 (0x00a0) - Program 7.8/16 FTF
PMT PID 176 (0x00b0) - Program 7.9/18 MTRSPT1
PMT PID 192 (0x00c0) - Program 7.10/20 NBT
PMT PID 208 (0x00d0) - Program 7.11/22 Bridge2
PMT PID 224 (0x00e0) - Program 7.12/24 DrOz
PMT PID 240 (0x00f0) - Program 7.13/26 beIN
PMT PID 256 (0x0100) - Program 7.14/28 ShopNow
PMT PID 272 (0x0110) - Program 7.15/30 Binge

### Program Map Table(s)

Program Number: 7.1/2 KDNU
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.2/4 Bridge1
PCR PID: 0x0041
Stream Type: 0x1b H.264 Video PID 65 (0x0041)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.3/6 InTouch
PCR PID: 0x0051
Stream Type: 0x1b H.264 Video PID 81 (0x0051)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.4/8 AWSN
PCR PID: 0x0061
Stream Type: 0x1b H.264 Video PID 97 (0x0061)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.5/10 Sales
PCR PID: 0x0071
Stream Type: 0x1b H.264 Video PID 113 (0x0071)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.6/12 BarkTV
PCR PID: 0x0081
Stream Type: 0x1b H.264 Video PID 129 (0x0081)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 132 (0x0084)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.7/14 ZLiving
PCR PID: 0x0091
Stream Type: 0x1b H.264 Video PID 145 (0x0091)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 148 (0x0094)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.8/16 FTF
PCR PID: 0x00a1
Stream Type: 0x1b H.264 Video PID 161 (0x00a1)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 164 (0x00a4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.9/18 MTRSPT1
PCR PID: 0x00b1
Stream Type: 0x1b H.264 Video PID 177 (0x00b1)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 180 (0x00b4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.10/20 NBT
PCR PID: 0x00c1
Stream Type: 0x1b H.264 Video PID 193 (0x00c1)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 196 (0x00c4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.11/22 Bridge2
PCR PID: 0x00d1
Stream Type: 0x1b H.264 Video PID 209 (0x00d1)
H.264 Video: Resolution 720 x 480 Interlaced: 1
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 212 (0x00d4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.12/24 DrOz
PCR PID: 0x00e1
Stream Type: 0x1b H.264 Video PID 225 (0x00e1)
H.264 Video: Resolution 720 x 480 Interlaced: 1
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 228 (0x00e4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.13/26 beIN
PCR PID: 0x00f1
Stream Type: 0x1b H.264 Video PID 241 (0x00f1)
H.264 Video: Resolution 720 x 480 Interlaced: 1
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 244 (0x00f4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.14/28 ShopNow
PCR PID: 0x0101
Stream Type: 0x1b H.264 Video PID 257 (0x0101)
H.264 Video: Resolution 720 x 480 Interlaced: 1
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 260 (0x0104)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 7.15/30 Binge
PCR PID: 0x0111
Stream Type: 0x1b H.264 Video PID 273 (0x0111)
H.264 Video: Resolution 720 x 480 Interlaced: 1
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 276 (0x0114)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

### Terrestrial Virtual Channel Table

Channel 2
Service Name: KDNU
TSID: 10851 (0x2a63)
Channel Number: 7.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng

Channel 4
Service Name: Bridge1
TSID: 10851 (0x2a63)
Channel Number: 7.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x1b (H.264 Video) ESPID = 0x0041 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 6
Service Name: InTouch
TSID: 10851 (0x2a63)
Channel Number: 7.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x1b (H.264 Video) ESPID = 0x0051 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 8
Service Name: AWSN
TSID: 10851 (0x2a63)
Channel Number: 7.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x1b (H.264 Video) ESPID = 0x0061 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 10
Service Name: Sales
TSID: 10851 (0x2a63)
Channel Number: 7.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x1b (H.264 Video) ESPID = 0x0071 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng

Channel 12
Service Name: BarkTV
TSID: 10851 (0x2a63)
Channel Number: 7.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0081
Stream Type 0x1b (H.264 Video) ESPID = 0x0081 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0084 Language = eng

Channel 14
Service Name: ZLiving
TSID: 10851 (0x2a63)
Channel Number: 7.7
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 7
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0091
Stream Type 0x1b (H.264 Video) ESPID = 0x0091 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0094 Language = eng

Channel 16
Service Name: FTF
TSID: 10851 (0x2a63)
Channel Number: 7.8
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 8
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00a1
Stream Type 0x1b (H.264 Video) ESPID = 0x00a1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00a4 Language = eng

Channel 18
Service Name: MTRSPT1
TSID: 10851 (0x2a63)
Channel Number: 7.9
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 9
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00b1
Stream Type 0x1b (H.264 Video) ESPID = 0x00b1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00b4 Language = eng

Channel 20
Service Name: NBT
TSID: 10851 (0x2a63)
Channel Number: 7.10
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 10
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00c1
Stream Type 0x1b (H.264 Video) ESPID = 0x00c1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00c4 Language = eng

Channel 22
Service Name: Bridge2
TSID: 10851 (0x2a63)
Channel Number: 7.11
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 11
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00d1
Stream Type 0x1b (H.264 Video) ESPID = 0x00d1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00d4 Language = eng

Channel 24
Service Name: DrOz
TSID: 10851 (0x2a63)
Channel Number: 7.12
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 12
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00e1
Stream Type 0x1b (H.264 Video) ESPID = 0x00e1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00e4 Language = eng

Channel 26
Service Name: beIN
TSID: 10851 (0x2a63)
Channel Number: 7.13
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 13
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00f1
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x00f1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00f4 Language = eng

Channel 28
Service Name: ShopNow
TSID: 10851 (0x2a63)
Channel Number: 7.14
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 14
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0101
Stream Type 0x1b (H.264 Video) ESPID = 0x0101 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0104 Language = eng

Channel 30
Service Name: Binge
TSID: 10851 (0x2a63)
Channel Number: 7.15
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 15
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0111
Stream Type 0x1b (H.264 Video) ESPID = 0x0111 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0114 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 803 | 0
CAT | 0 | 0
PMT | 30 | 0
ETT | 0 | 0
PSIP | 1.1k | 0
EIT | 0 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,753 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 30 (569 MHz)
Signal: Locked Signal 83 Quality 54
Network Type: ATSC
Run Time: 000:01:09

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.05% ~ 0.01 Mbps) |  | 0x0030 MPEG-2 PMT for program 7.1/2
0x0031 (11.12% - 3.10 Mbps) |  | 0x0031 MPEG-2 Video for program 7.1/2
0x0034 (0.73% ~ 0.14 Mbps) |  | 0x0034 AC-3 Audio for program 7.1/2
0x0040 (0.05% ~ 0.01 Mbps) |  | 0x0040 MPEG-2 PMT for program 7.2/4
0x0041 (4.66% - 1.32 Mbps) |  | 0x0041 H.264 Video for program 7.2/4
0x0044 (0.73% ~ 0.14 Mbps) |  | 0x0044 AC-3 Audio for program 7.2/4
0x0050 (0.05% ~ 0.01 Mbps) |  | 0x0050 MPEG-2 PMT for program 7.3/6
0x0051 (4.40% - 1.41 Mbps) |  | 0x0051 H.264 Video for program 7.3/6
0x0054 (0.73% ~ 0.14 Mbps) |  | 0x0054 AC-3 Audio for program 7.3/6
0x0060 (0.05% ~ 0.01 Mbps) |  | 0x0060 MPEG-2 PMT for program 7.4/8
0x0061 (5.42% - 1.54 Mbps) |  | 0x0061 H.264 Video for program 7.4/8
0x0064 (0.73% ~ 0.14 Mbps) |  | 0x0064 AC-3 Audio for program 7.4/8
0x0070 (0.05% ~ 0.01 Mbps) |  | 0x0070 MPEG-2 PMT for program 7.5/10
0x0071 (4.35% - 1.48 Mbps) |  | 0x0071 H.264 Video for program 7.5/10
0x0074 (0.73% ~ 0.14 Mbps) |  | 0x0074 AC-3 Audio for program 7.5/10
0x0080 (0.05% ~ 0.01 Mbps) |  | 0x0080 MPEG-2 PMT for program 7.6/12
0x0081 (5.12% - 1.72 Mbps) |  | 0x0081 H.264 Video for program 7.6/12
0x0084 (0.73% ~ 0.14 Mbps) |  | 0x0084 AC-3 Audio for program 7.6/12
0x0090 (0.05% ~ 0.01 Mbps) |  | 0x0090 MPEG-2 PMT for program 7.7/14
0x0091 (4.70% - 1.47 Mbps) |  | 0x0091 H.264 Video for program 7.7/14
0x0094 (0.73% ~ 0.14 Mbps) |  | 0x0094 AC-3 Audio for program 7.7/14
0x00a0 (0.05% ~ 0.01 Mbps) |  | 0x00a0 MPEG-2 PMT for program 7.8/16
0x00a1 (5.31% - 1.62 Mbps) |  | 0x00a1 H.264 Video for program 7.8/16
0x00a4 (0.73% ~ 0.14 Mbps) |  | 0x00a4 AC-3 Audio for program 7.8/16
0x00b0 (0.05% ~ 0.01 Mbps) |  | 0x00b0 MPEG-2 PMT for program 7.9/18
0x00b1 (5.47% - 1.71 Mbps) |  | 0x00b1 H.264 Video for program 7.9/18
0x00b4 (0.73% ~ 0.14 Mbps) |  | 0x00b4 AC-3 Audio for program 7.9/18
0x00c0 (0.05% ~ 0.01 Mbps) |  | 0x00c0 MPEG-2 PMT for program 7.10/20
0x00c1 (4.81% - 1.37 Mbps) |  | 0x00c1 H.264 Video for program 7.10/20
0x00c4 (0.73% ~ 0.14 Mbps) |  | 0x00c4 AC-3 Audio for program 7.10/20
0x00d0 (0.05% ~ 0.01 Mbps) |  | 0x00d0 MPEG-2 PMT for program 7.11/22
0x00d1 (4.41% - 1.46 Mbps) |  | 0x00d1 H.264 Video for program 7.11/22
0x00d4 (0.73% ~ 0.14 Mbps) |  | 0x00d4 AC-3 Audio for program 7.11/22
0x00e0 (0.05% ~ 0.01 Mbps) |  | 0x00e0 MPEG-2 PMT for program 7.12/24
0x00e1 (4.45% - 1.36 Mbps) |  | 0x00e1 H.264 Video for program 7.12/24
0x00e4 (0.73% ~ 0.14 Mbps) |  | 0x00e4 AC-3 Audio for program 7.12/24
0x00f0 (0.05% ~ 0.01 Mbps) |  | 0x00f0 MPEG-2 PMT for program 7.13/26
0x00f1 (5.33% - 1.67 Mbps) |  | 0x00f1 H.264 Video for program 7.13/26
0x00f4 (0.73% ~ 0.14 Mbps) |  | 0x00f4 AC-3 Audio for program 7.13/26
0x0100 (0.05% ~ 0.01 Mbps) |  | 0x0100 MPEG-2 PMT for program 7.14/28
0x0101 (4.43% - 1.52 Mbps) |  | 0x0101 H.264 Video for program 7.14/28
0x0104 (0.73% ~ 0.14 Mbps) |  | 0x0104 AC-3 Audio for program 7.14/28
0x0110 (0.05% ~ 0.01 Mbps) |  | 0x0110 MPEG-2 PMT for program 7.15/30
0x0111 (4.39% - 1.26 Mbps) |  | 0x0111 H.264 Video for program 7.15/30
0x0114 (0.73% ~ 0.14 Mbps) |  | 0x0114 AC-3 Audio for program 7.15/30
0x1ffb (0.21% ~ 0.04 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (9.62% ~ 1.86 Mbps) |  | 0x1fff MPEG-2 NULL Packet