### Program Association Table

PAT Version Number: 1
Transport Stream ID: 223 (0x00df)
PMT PID 48 (0x0030) - Program 27.1/1 PBS HD
PMT PID 64 (0x0040) - Program 27.2/2 KIDS
PMT PID 80 (0x0050) - Program 27.3/3 PBS 6+
PMT PID 96 (0x0060) - Program 40.11/4 KHRR-DT
PMT PID 112 (0x0070) - Program 40.21/5 Exitos

### Program Map Table(s)

Program Number: 27.1/1 PBS HD
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 0.960 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 384 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 3/2 5 L, C, R, SL, SR
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Stream Type: 0x81 AC-3 Audio PID 56 (0x0038)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode visually impaired Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 27.2/2 KIDS
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 0.470 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Stream Type: 0x81 AC-3 Audio PID 72 (0x0048)
AC3: Bitrate 96 Kbps Sample Rate 48 KHz
AC3: Mode visually impaired Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 27.3/3 PBS 6+
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 2.917 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Stream Type: 0x81 AC-3 Audio PID 88 (0x0058)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode visually impaired Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 40.11/4 KHRR-DT
Descriptor: Registration Descriptor
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 9.768 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 384 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 3/2 5 L, C, R, SL, SR
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor
Stream Type: 0x81 AC-3 Audio PID 101 (0x0065)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode visually impaired Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 40.21/5 Exitos
Descriptor: Registration Descriptor
Descriptor: ATSC Content Advisory Descriptor
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 0.470 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: PBS HD
TSID: 223 (0x00df) Old-NTSC: 27 ATSC: 28 AZ TUCSON
Channel Number: 27.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0038 Language = eng

Channel 2
Service Name: KIDS
TSID: 223 (0x00df) Old-NTSC: 27 ATSC: 28 AZ TUCSON
Channel Number: 27.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0048 Language = fra

Channel 3
Service Name: PBS 6+
TSID: 223 (0x00df) Old-NTSC: 27 ATSC: 28 AZ TUCSON
Channel Number: 27.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0058 Language = eng

Channel 4
Service Name: KHRR-DT
TSID: 223 (0x00df) Old-NTSC: 27 ATSC: 28 AZ TUCSON
Channel Number: 40.11
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = spa
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0065 Language = spa

Channel 5
Service Name: Exitos
TSID: 223 (0x00df) Old-NTSC: 27 ATSC: 28 AZ TUCSON
Channel Number: 40.21
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = spa

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 787 | 0
CAT | 0 | 0
PMT | 10 | 0
ETT | 6.2k | 0
PSIP | 1.1k | 0
EIT | 1.4k | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,669 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 28 (557 MHz)
Signal: Locked Signal 50 Quality 51
Network Type: ATSC
Run Time: 000:01:13

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.03% ~ 0.01 Mbps) |  | 0x0030 MPEG-2 PMT for program 27.1/1
0x0031 (25.69% - 4.98 Mbps) |  | 0x0031 MPEG-2 Video for program 27.1/1
0x0034 (2.06% ~ 0.40 Mbps) |  | 0x0034 AC-3 Audio for program 27.1/1
0x0036 (0.71% ~ 0.14 Mbps) |  | 0x0036 Unknown usage
0x0037 (0.72% ~ 0.14 Mbps) |  | 0x0037 Unknown usage
0x0038 (1.05% ~ 0.20 Mbps) |  | 0x0038 AC-3 Audio for program 27.1/1
0x0040 (0.03% ~ 0.01 Mbps) |  | 0x0040 MPEG-2 PMT for program 27.2/2
0x0041 (5.64% - 1.09 Mbps) |  | 0x0041 MPEG-2 Video for program 27.2/2
0x0044 (1.05% ~ 0.20 Mbps) |  | 0x0044 AC-3 Audio for program 27.2/2
0x0048 (0.53% ~ 0.10 Mbps) |  | 0x0048 AC-3 Audio for program 27.2/2
0x0050 (0.03% ~ 0.01 Mbps) |  | 0x0050 MPEG-2 PMT for program 27.3/3
0x0051 (5.51% - 1.07 Mbps) |  | 0x0051 MPEG-2 Video for program 27.3/3
0x0054 (1.05% ~ 0.20 Mbps) |  | 0x0054 AC-3 Audio for program 27.3/3
0x0058 (1.05% ~ 0.20 Mbps) |  | 0x0058 AC-3 Audio for program 27.3/3
0x0060 (0.03% ~ 0.01 Mbps) |  | 0x0060 MPEG-2 PMT for program 40.11/4
0x0061 (39.75% - 7.71 Mbps) |  | 0x0061 MPEG-2 Video for program 40.11/4
0x0064 (2.06% ~ 0.40 Mbps) |  | 0x0064 AC-3 Audio for program 40.11/4
0x0065 (1.05% ~ 0.20 Mbps) |  | 0x0065 AC-3 Audio for program 40.11/4
0x0070 (0.03% ~ 0.01 Mbps) |  | 0x0070 MPEG-2 PMT for program 40.21/5
0x0071 (6.44% - 1.25 Mbps) |  | 0x0071 MPEG-2 Video for program 40.21/5
0x0074 (1.05% ~ 0.20 Mbps) |  | 0x0074 AC-3 Audio for program 40.21/5
0x0911 (0.00% ~ 0.00 Mbps) |  | 0x0911 Unknown usage
0x1d00 (0.27% ~ 0.05 Mbps) |  | 0x1d00 ATSC EIT-0
0x1d01 (0.06% ~ 0.01 Mbps) |  | 0x1d01 ATSC EIT-1
0x1d02 (0.03% ~ 0.01 Mbps) |  | 0x1d02 ATSC EIT-2
0x1d03 (0.02% ~ 0.00 Mbps) |  | 0x1d03 ATSC EIT-3
0x1e00 (0.63% ~ 0.12 Mbps) |  | 0x1e00 ATSC Event ETT-0
0x1e01 (0.14% ~ 0.03 Mbps) |  | 0x1e01 ATSC Event ETT-1
0x1e02 (0.06% ~ 0.01 Mbps) |  | 0x1e02 ATSC Event ETT-2
0x1e03 (0.05% ~ 0.01 Mbps) |  | 0x1e03 ATSC Event ETT-3
0x1ffb (0.18% ~ 0.03 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (2.96% ~ 0.57 Mbps) |  | 0x1fff MPEG-2 NULL Packet