### Program Association Table

PAT Version Number: 1
Transport Stream ID: 10841 (0x2a59)
PMT PID 48 (0x0030) - Program 23.1/1 KLVD-LD
PMT PID 64 (0x0040) - Program 23.2/2 ESPANOL
PMT PID 80 (0x0050) - Program 23.3/3 KLVD-3

### Program Map Table(s)

Program Number: 23.1/1 KLVD-LD
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 14.172 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 448 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 3/2 5 L, C, R, SL, SR
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: Registration Descriptor
Stream Type: 0x81 AC-3 Audio PID 53 (0x0035)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode visually impaired Coding 2/0 L, R
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: Registration Descriptor

Program Number: 23.2/2 ESPANOL
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 14.164 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: Registration Descriptor

Program Number: 23.3/3 KLVD-3
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 2.917 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: Registration Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: KLVD-LD
TSID: 10841 (0x2a59)
Channel Number: 23.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0035 Language = eng

Channel 2
Service Name: ESPANOL
TSID: 10841 (0x2a59)
Channel Number: 23.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 3
Service Name: KLVD-3
TSID: 10841 (0x2a59)
Channel Number: 23.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 488 | 0
CAT | 0 | 0
PMT | 6 | 0
ETT | 0 | 0
PSIP | 486 | 0
EIT | 0 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,385,992 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 23 (527 MHz)
Signal: Locked Signal 100 Quality 81
Network Type: ATSC
Run Time: 000:00:44

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.09% ~ 0.02 Mbps) |  | 0x0030 MPEG-2 PMT for program 23.1/1
0x0031 (37.16% - 7.21 Mbps) |  | 0x0031 MPEG-2 Video for program 23.1/1
0x0034 (2.38% ~ 0.46 Mbps) |  | 0x0034 AC-3 Audio for program 23.1/1
0x0035 (1.02% ~ 0.20 Mbps) |  | 0x0035 AC-3 Audio for program 23.1/1
0x0040 (0.09% ~ 0.02 Mbps) |  | 0x0040 MPEG-2 PMT for program 23.2/2
0x0041 (39.86% - 7.74 Mbps) |  | 0x0041 MPEG-2 Video for program 23.2/2
0x0044 (1.02% ~ 0.20 Mbps) |  | 0x0044 AC-3 Audio for program 23.2/2
0x0050 (0.09% ~ 0.02 Mbps) |  | 0x0050 MPEG-2 PMT for program 23.3/3
0x0051 (6.01% - 1.17 Mbps) |  | 0x0051 MPEG-2 Video for program 23.3/3
0x0054 (1.02% ~ 0.20 Mbps) |  | 0x0054 AC-3 Audio for program 23.3/3
0x1ffb (0.08% ~ 0.02 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (11.11% ~ 2.15 Mbps) |  | 0x1fff MPEG-2 NULL Packet