### Program Association Table

PAT Version Number: 6
Transport Stream ID: 211 (0x00d3)
PMT PID 48 (0x0030) - Program 4.1/1 KVOANBC
PMT PID 64 (0x0040) - Program 4.2/2 COZI
PMT PID 80 (0x0050) - Program 4.3/3 MYSTERY
PMT PID 96 (0x0060) - Program 4.4/4 MeToons
PMT PID 144 (0x0090) - Program 40.3/7 NBC LX

### Program Map Table(s)

Program Number: 4.1/1 KVOANBC
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 17.598 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 384 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 3/2 5 L, C, R, SL, SR
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x81 AC-3 Audio PID 53 (0x0035)
AC3: Bitrate 96 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 4.2/2 COZI
PCR PID: 0x0041
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 2.917 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: ATSC Caption Service Descriptor

Program Number: 4.3/3 MYSTERY
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 2.917 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 4.4/4 MeToons
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 2.917 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 40.3/7 NBC LX
PCR PID: 0x0091
Stream Type: 0x02 MPEG-2 Video PID 145 (0x0091)
MPEG Video: Bitrate 7.811 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: ATSC Caption Service Descriptor
Stream Type: 0x81 AC-3 Audio PID 148 (0x0094)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: KVOANBC
TSID: 211 (0x00d3) Old-NTSC: 04 ATSC: 23 AZ TUCSON
Channel Number: 4.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0035 Language = spa

Channel 2
Service Name: COZI
TSID: 211 (0x00d3) Old-NTSC: 04 ATSC: 23 AZ TUCSON
Channel Number: 4.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =

Channel 3
Service Name: MYSTERY
TSID: 211 (0x00d3) Old-NTSC: 04 ATSC: 23 AZ TUCSON
Channel Number: 4.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 4
Service Name: MeToons
TSID: 211 (0x00d3) Old-NTSC: 04 ATSC: 23 AZ TUCSON
Channel Number: 4.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 7
Service Name: NBC LX
TSID: 211 (0x00d3) Old-NTSC: 04 ATSC: 23 AZ TUCSON
Channel Number: 40.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 7
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0091
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0091 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0094 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 1.8k | 0
CAT | 0 | 0
PMT | 10 | 0
ETT | 1.0k | 0
PSIP | 1.7k | 0
EIT | 2.4k | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,571 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 17 (491 MHz)
Signal: Locked Signal 72 Quality 76
Network Type: ATSC
Run Time: 000:02:25

### PID Usage Chart

0x0000 (0.10% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.03% ~ 0.01 Mbps) |  | 0x0030 MPEG-2 PMT for program 4.1/1
0x0031 (45.68% - 8.86 Mbps) |  | 0x0031 MPEG-2 Video for program 4.1/1
0x0034 (2.04% ~ 0.39 Mbps) |  | 0x0034 AC-3 Audio for program 4.1/1
0x0035 (0.53% ~ 0.10 Mbps) |  | 0x0035 AC-3 Audio for program 4.1/1
0x0040 (0.03% ~ 0.01 Mbps) |  | 0x0040 MPEG-2 PMT for program 4.2/2
0x0041 (10.17% - 1.97 Mbps) |  | 0x0041 MPEG-2 Video for program 4.2/2
0x0044 (1.02% ~ 0.20 Mbps) |  | 0x0044 AC-3 Audio for program 4.2/2
0x0050 (0.03% ~ 0.01 Mbps) |  | 0x0050 MPEG-2 PMT for program 4.3/3
0x0051 (10.63% - 2.06 Mbps) |  | 0x0051 MPEG-2 Video for program 4.3/3
0x0054 (1.02% ~ 0.20 Mbps) |  | 0x0054 AC-3 Audio for program 4.3/3
0x0060 (0.03% ~ 0.01 Mbps) |  | 0x0060 MPEG-2 PMT for program 4.4/4
0x0061 (9.72% - 1.89 Mbps) |  | 0x0061 MPEG-2 Video for program 4.4/4
0x0064 (1.02% ~ 0.20 Mbps) |  | 0x0064 AC-3 Audio for program 4.4/4
0x0090 (0.03% ~ 0.01 Mbps) |  | 0x0090 MPEG-2 PMT for program 40.3/7
0x0091 (9.64% - 1.87 Mbps) |  | 0x0091 MPEG-2 Video for program 40.3/7
0x0094 (1.02% ~ 0.20 Mbps) |  | 0x0094 AC-3 Audio for program 40.3/7
0x1d00 (0.11% ~ 0.02 Mbps) |  | 0x1d00 ATSC EIT-0
0x1d01 (0.03% ~ 0.01 Mbps) |  | 0x1d01 ATSC EIT-1
0x1d02 (0.02% ~ 0.00 Mbps) |  | 0x1d02 ATSC EIT-2
0x1d03 (0.01% ~ 0.00 Mbps) |  | 0x1d03 ATSC EIT-3
0x1e00 (0.02% ~ 0.00 Mbps) |  | 0x1e00 ATSC Event ETT-0
0x1e01 (0.01% ~ 0.00 Mbps) |  | 0x1e01 ATSC Event ETT-1
0x1e02 (0.02% ~ 0.00 Mbps) |  | 0x1e02 ATSC Event ETT-2
0x1e03 (0.01% ~ 0.00 Mbps) |  | 0x1e03 ATSC Event ETT-3
0x1ffb (0.12% ~ 0.02 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (6.96% ~ 1.35 Mbps) |  | 0x1fff MPEG-2 NULL Packet