### Program Association Table

PAT Version Number: 1
Transport Stream ID: 0 (0x0000)
PMT PID 181 (0x00b5) - Program 50.1/1 ShopLC
PMT PID 51 (0x0033) - Program 50.6/2 JTV
PMT PID 54 (0x0036) - Program 50.4/4 The Can
PMT PID 57 (0x0039) - Program 50.5/5 AllStar
PMT PID 60 (0x003c) - Program 50.3/6 Quinnly
PMT PID 4096 (0x1000) - Program 50.2/7 Peak TV

### Program Map Table(s)

Program Number: 50.1/1 ShopLC
PCR PID: 0x0263
Stream Type: 0x81 AC-3 Audio PID 131 (0x0083)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x02 MPEG-2 Video PID 611 (0x0263)
MPEG Video: Bitrate 15.000 Mbps Resolution 544 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 50.6/2 JTV
PCR PID: 0x00d2
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x02 MPEG-2 Video PID 53 (0x0035)
MPEG Video: Bitrate 15.000 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Descriptor: Reserved: 0x00

Program Number: 50.4/4 The Can
PCR PID: 0x0037
Stream Type: 0x02 MPEG-2 Video PID 55 (0x0037)
MPEG Video: Bitrate 104.857 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 30 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 56 (0x0038)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor

Program Number: 50.5/5 AllStar
PCR PID: 0x003a
Stream Type: 0x02 MPEG-2 Video PID 58 (0x003a)
MPEG Video: Bitrate 104.857 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 30 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 59 (0x003b)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor

Program Number: 50.3/6 Quinnly
PCR PID: 0x0103
Stream Type: 0x02 MPEG-2 Video PID 61 (0x003d)
MPEG Video: Bitrate 2.700 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 258 (0x0102)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 50.2/7 Peak TV
PCR PID: 0x0100
Stream Type: 0x02 MPEG-2 Video PID 256 (0x0100)
MPEG Video: Bitrate 104.857 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 30 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 257 (0x0101)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: ShopLC
TSID: 0 (0x0000)
Channel Number: 50.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0263
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0083 Language = eng
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0263 Language = eng

Channel 2
Service Name: JTV
TSID: 0 (0x0000)
Channel Number: 50.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00d2
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0035 Language = eng

Channel 4
Service Name: The Can
TSID: 0 (0x0000)
Channel Number: 50.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0037
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0037 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0038 Language = eng

Channel 5
Service Name: AllStar
TSID: 0 (0x0000)
Channel Number: 50.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x003a
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x003a Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x003b Language = eng

Channel 6
Service Name: Quinnly
TSID: 0 (0x0000)
Channel Number: 50.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0103
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x003d Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0102 Language = eng

Channel 7
Service Name: Peak TV
TSID: 0 (0x0000)
Channel Number: 50.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0100
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0100 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0101 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 550 | 0
CAT | 0 | 0
PMT | 12 | 0
ETT | 0 | 0
PSIP | 551 | 0
EIT | 0 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,393,889 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 21 (515 MHz)
Signal: Locked Signal 100 Quality 69
Network Type: ATSC
Run Time: 000:00:50

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0033 (0.09% ~ 0.02 Mbps) |  | 0x0033 MPEG-2 PMT for program 50.6/2
0x0034 (1.02% ~ 0.20 Mbps) |  | 0x0034 AC-3 Audio for program 50.6/2
0x0035 (10.31% - 2.06 Mbps) |  | 0x0035 MPEG-2 Video for program 50.6/2
0x0036 (0.09% ~ 0.02 Mbps) |  | 0x0036 MPEG-2 PMT for program 50.4/4
0x0037 (8.09% - 1.55 Mbps) |  | 0x0037 MPEG-2 Video for program 50.4/4
0x0038 (1.21% ~ 0.23 Mbps) |  | 0x0038 AC-3 Audio for program 50.4/4
0x0039 (0.09% ~ 0.02 Mbps) |  | 0x0039 MPEG-2 PMT for program 50.5/5
0x003a (4.04% - 0.86 Mbps) |  | 0x003a MPEG-2 Video for program 50.5/5
0x003b (1.21% ~ 0.23 Mbps) |  | 0x003b AC-3 Audio for program 50.5/5
0x003c (0.09% ~ 0.02 Mbps) |  | 0x003c MPEG-2 PMT for program 50.3/6
0x003d (16.43% ~ 3.19 Mbps) |  | 0x003d MPEG-2 Video for program 50.3/6
0x0083 (1.02% ~ 0.20 Mbps) |  | 0x0083 AC-3 Audio for program 50.1/1
0x00b5 (0.09% ~ 0.02 Mbps) |  | 0x00b5 MPEG-2 PMT for program 50.1/1
0x0100 (8.01% - 1.92 Mbps) |  | 0x0100 MPEG-2 Video for program 50.2/7
0x0101 (1.21% ~ 0.24 Mbps) |  | 0x0101 AC-3 Audio for program 50.2/7
0x0102 (1.21% ~ 0.24 Mbps) |  | 0x0102 AC-3 Audio for program 50.3/6
0x0103 (0.26% - 0.05 Mbps) |  | 0x0103 MPEG-2 PCR for program 50.3/6
0x0263 (7.73% - 1.57 Mbps) |  | 0x0263 MPEG-2 Video for program 50.1/1
0x1000 (0.09% ~ 0.02 Mbps) |  | 0x1000 MPEG-2 PMT for program 50.2/7
0x1ffb (0.11% ~ 0.02 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (37.54% ~ 7.28 Mbps) |  | 0x1fff MPEG-2 NULL Packet