### Program Association Table

PAT Version Number: 1
Transport Stream ID: 2093 (0x082d)
PMT PID 48 (0x0030) - Program 39.1/3 KBLR-HD
PMT PID 64 (0x0040) - Program 39.2/4 TelEx
PMT PID 80 (0x0050) - Program 39.3/5 CRIMES
PMT PID 96 (0x0060) - Program 39.4/6 COZI
PMT PID 112 (0x0070) - Program 39.5/7 Oxygen
PMT PID 128 (0x0080) - Program 39.6/8 Nosey

### Program Map Table(s)

Program Number: 39.1/3 KBLR-HD
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 13.683 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 224 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 3/2 5 L, C, R, SL, SR
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 39.2/4 TelEx
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 5.854 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 39.3/5 CRIMES
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 5.854 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 39.4/6 COZI
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 5.854 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 39.5/7 Oxygen
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 5.854 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 39.6/8 Nosey
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0081
Stream Type: 0x02 MPEG-2 Video PID 129 (0x0081)
MPEG Video: Bitrate 5.854 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 132 (0x0084)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 3
Service Name: KBLR-HD
TSID: 2093 (0x082d) VCh: 39 RFCh: 20 KBLR PARADISE, NV
Channel Number: 39.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = spa

Channel 4
Service Name: TelEx
TSID: 2093 (0x082d) VCh: 39 RFCh: 20 KBLR PARADISE, NV
Channel Number: 39.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = spa

Channel 5
Service Name: CRIMES
TSID: 2093 (0x082d) VCh: 39 RFCh: 20 KBLR PARADISE, NV
Channel Number: 39.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 6
Service Name: COZI
TSID: 2093 (0x082d) VCh: 39 RFCh: 20 KBLR PARADISE, NV
Channel Number: 39.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 7
Service Name: Oxygen
TSID: 2093 (0x082d) VCh: 39 RFCh: 20 KBLR PARADISE, NV
Channel Number: 39.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 7
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng

Channel 8
Service Name: Nosey
TSID: 2093 (0x082d) VCh: 39 RFCh: 20 KBLR PARADISE, NV
Channel Number: 39.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 8
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0081
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0081 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0084 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 716 | 0
CAT | 0 | 0
PMT | 12 | 0
ETT | 276 | 0
PSIP | 901 | 0
EIT | 1.1k | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,654 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 20 (509 MHz)
Signal: Locked Signal 100 Quality 83
Network Type: ATSC
Run Time: 000:01:02

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.09% ~ 0.02 Mbps) |  | 0x0030 MPEG-2 PMT for program 39.1/3
0x0031 (40.33% - 7.81 Mbps) |  | 0x0031 MPEG-2 Video for program 39.1/3
0x0034 (1.21% ~ 0.23 Mbps) |  | 0x0034 AC-3 Audio for program 39.1/3
0x0040 (0.09% ~ 0.02 Mbps) |  | 0x0040 MPEG-2 PMT for program 39.2/4
0x0041 (8.24% - 1.60 Mbps) |  | 0x0041 MPEG-2 Video for program 39.2/4
0x0044 (1.02% ~ 0.20 Mbps) |  | 0x0044 AC-3 Audio for program 39.2/4
0x0050 (0.09% ~ 0.02 Mbps) |  | 0x0050 MPEG-2 PMT for program 39.3/5
0x0051 (7.66% - 1.48 Mbps) |  | 0x0051 MPEG-2 Video for program 39.3/5
0x0054 (1.02% ~ 0.20 Mbps) |  | 0x0054 AC-3 Audio for program 39.3/5
0x0060 (0.09% ~ 0.02 Mbps) |  | 0x0060 MPEG-2 PMT for program 39.4/6
0x0061 (6.69% - 1.30 Mbps) |  | 0x0061 MPEG-2 Video for program 39.4/6
0x0064 (1.02% ~ 0.20 Mbps) |  | 0x0064 AC-3 Audio for program 39.4/6
0x0070 (0.09% ~ 0.02 Mbps) |  | 0x0070 MPEG-2 PMT for program 39.5/7
0x0071 (7.34% - 1.42 Mbps) |  | 0x0071 MPEG-2 Video for program 39.5/7
0x0074 (1.02% ~ 0.20 Mbps) |  | 0x0074 AC-3 Audio for program 39.5/7
0x0080 (0.09% ~ 0.02 Mbps) |  | 0x0080 MPEG-2 PMT for program 39.6/8
0x0081 (5.52% - 1.07 Mbps) |  | 0x0081 MPEG-2 Video for program 39.6/8
0x0084 (1.02% ~ 0.20 Mbps) |  | 0x0084 AC-3 Audio for program 39.6/8
0x1388 (0.22% ~ 0.04 Mbps) |  | 0x1388 ATSC EIT-0
0x1389 (0.04% ~ 0.01 Mbps) |  | 0x1389 ATSC EIT-1
0x138a (0.01% ~ 0.00 Mbps) |  | 0x138a ATSC EIT-2
0x138b (0.01% ~ 0.00 Mbps) |  | 0x138b ATSC EIT-3
0x1408 (0.01% ~ 0.00 Mbps) |  | 0x1408 ATSC Event ETT-0
0x1409 (0.01% ~ 0.00 Mbps) |  | 0x1409 ATSC Event ETT-1
0x140a (0.01% ~ 0.00 Mbps) |  | 0x140a ATSC Event ETT-2
0x140b (0.01% ~ 0.00 Mbps) |  | 0x140b ATSC Event ETT-3
0x1ffb (0.14% ~ 0.03 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (16.84% ~ 3.27 Mbps) |  | 0x1fff MPEG-2 NULL Packet