### Program Association Table

PAT Version Number: 1
Transport Stream ID: 10187 (0x27cb)
PMT PID 48 (0x0030) - Program 51.1/2 KVGA-LD
PMT PID 64 (0x0040) - Program 51.2/4 RTV
PMT PID 80 (0x0050) - Program 51.3/6 REVN
PMT PID 96 (0x0060) - Program 51.4/8 Action
PMT PID 112 (0x0070) - Program 51.5/10 Family
PMT PID 128 (0x0080) - Program 51.6/12 Revival
PMT PID 144 (0x0090) - Program 51.7/14 GLTVii

### Program Map Table(s)

Program Number: 51.1/2 KVGA-LD
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 38.000 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 51.2/4 RTV
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 51.3/6 REVN
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 51.4/8 Action
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 51.5/10 Family
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 51.6/12 Revival
PCR PID: 0x0081
Stream Type: 0x02 MPEG-2 Video PID 129 (0x0081)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 132 (0x0084)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 51.7/14 GLTVii
PCR PID: 0x0091
Stream Type: 0x02 MPEG-2 Video PID 145 (0x0091)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 148 (0x0094)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

### Terrestrial Virtual Channel Table

Channel 2
Service Name: KVGA-LD
TSID: 10187 (0x27cb)
Channel Number: 51.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng

Channel 4
Service Name: RTV
TSID: 10187 (0x27cb)
Channel Number: 51.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 6
Service Name: REVN
TSID: 10187 (0x27cb)
Channel Number: 51.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 8
Service Name: Action
TSID: 10187 (0x27cb)
Channel Number: 51.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 10
Service Name: Family
TSID: 10187 (0x27cb)
Channel Number: 51.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng

Channel 12
Service Name: Revival
TSID: 10187 (0x27cb)
Channel Number: 51.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0081
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0081 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0084 Language = eng

Channel 14
Service Name: GLTVii
TSID: 10187 (0x27cb)
Channel Number: 51.7
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 7
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0091
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0091 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0094 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 1000 | 0
CAT | 0 | 0
PMT | 14 | 0
ETT | 9.4k | 0
PSIP | 1.0k | 0
EIT | 2.8k | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,696 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 12 (207 MHz)
Signal: Locked Signal 95 Quality 68
Network Type: ATSC
Run Time: 000:01:25

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.04% ~ 0.01 Mbps) |  | 0x0030 MPEG-2 PMT for program 51.1/2
0x0031 (28.52% - 9.64 Mbps) |  | 0x0031 MPEG-2 Video for program 51.1/2
0x0034 (1.21% ~ 0.23 Mbps) |  | 0x0034 AC-3 Audio for program 51.1/2
0x0040 (0.04% ~ 0.01 Mbps) |  | 0x0040 MPEG-2 PMT for program 51.2/4
0x0041 (8.99% - 2.37 Mbps) |  | 0x0041 MPEG-2 Video for program 51.2/4
0x0044 (0.73% ~ 0.14 Mbps) |  | 0x0044 AC-3 Audio for program 51.2/4
0x0050 (0.04% ~ 0.01 Mbps) |  | 0x0050 MPEG-2 PMT for program 51.3/6
0x0051 (9.16% - 2.38 Mbps) |  | 0x0051 MPEG-2 Video for program 51.3/6
0x0054 (0.73% ~ 0.14 Mbps) |  | 0x0054 AC-3 Audio for program 51.3/6
0x0060 (0.04% ~ 0.01 Mbps) |  | 0x0060 MPEG-2 PMT for program 51.4/8
0x0061 (9.92% - 2.97 Mbps) |  | 0x0061 MPEG-2 Video for program 51.4/8
0x0070 (0.04% ~ 0.01 Mbps) |  | 0x0070 MPEG-2 PMT for program 51.5/10
0x0071 (7.87% - 1.96 Mbps) |  | 0x0071 MPEG-2 Video for program 51.5/10
0x0074 (0.73% ~ 0.14 Mbps) |  | 0x0074 AC-3 Audio for program 51.5/10
0x0080 (0.04% ~ 0.01 Mbps) |  | 0x0080 MPEG-2 PMT for program 51.6/12
0x0081 (10.42% - 2.95 Mbps) |  | 0x0081 MPEG-2 Video for program 51.6/12
0x0084 (1.21% ~ 0.24 Mbps) |  | 0x0084 AC-3 Audio for program 51.6/12
0x0090 (0.04% ~ 0.01 Mbps) |  | 0x0090 MPEG-2 PMT for program 51.7/14
0x0091 (13.02% - 3.68 Mbps) |  | 0x0091 MPEG-2 Video for program 51.7/14
0x0094 (1.21% ~ 0.24 Mbps) |  | 0x0094 AC-3 Audio for program 51.7/14
0x1e00 (0.29% ~ 0.06 Mbps) |  | 0x1e00 ATSC EIT-0
0x1e01 (0.07% ~ 0.01 Mbps) |  | 0x1e01 ATSC EIT-1
0x1e02 (0.00% ~ 0.00 Mbps) |  | 0x1e02 ATSC EIT-2
0x1e03 (0.00% ~ 0.00 Mbps) |  | 0x1e03 ATSC EIT-3
0x1e80 (0.73% ~ 0.14 Mbps) |  | 0x1e80 ATSC Event ETT-0
0x1e81 (0.16% ~ 0.03 Mbps) |  | 0x1e81 ATSC Event ETT-1
0x1e82 (0.01% ~ 0.00 Mbps) |  | 0x1e82 ATSC Event ETT-2
0x1e83 (0.01% ~ 0.00 Mbps) |  | 0x1e83 ATSC Event ETT-3
0x1ffb (0.12% ~ 0.02 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (4.52% ~ 0.88 Mbps) |  | 0x1fff MPEG-2 NULL Packet