### Program Association Table

PAT Version Number: 0
Transport Stream ID: 8759 (0x2237)
PMT PID 48 (0x0030) - Program 17.1/3 KEEN
PMT PID 80 (0x0050) - Program 17.3/5 CTNi
PMT PID 112 (0x0070) - Program 17.5/7 BIZ-TV

### Program Map Table(s)

Program Number: 17.1/3 KEEN
Descriptor: Smoothing Buffer Descriptor
Descriptor: ATSC Content Advisory Descriptor
Descriptor: Registration Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 27.438 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: ATSC Caption Service Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 17.3/5 CTNi
Descriptor: Smoothing Buffer Descriptor
Descriptor: ATSC Content Advisory Descriptor
Descriptor: Registration Descriptor
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 15.000 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Descriptor: ATSC Caption Service Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 17.5/7 BIZ-TV
Descriptor: Smoothing Buffer Descriptor
Descriptor: ATSC Content Advisory Descriptor
Descriptor: Registration Descriptor
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 15.000 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 4:3
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 3
Service Name: KEEN
TSID: 8759 (0x2237) VCh: 17 RFCh: 17 KEEN-CD LAS VEGAS, NV
Channel Number: 17.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 16
Descriptor: ATSC Extended Channel Name Descriptor
Extended Channel Name: CTN-Las Vegas
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language =

Channel 5
Service Name: CTNi
TSID: 8759 (0x2237) VCh: 17 RFCh: 17 KEEN-CD LAS VEGAS, NV
Channel Number: 17.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 18
Descriptor: ATSC Extended Channel Name Descriptor
Extended Channel Name: Christian Television International
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language =

Channel 7
Service Name: BIZ-TV
TSID: 8759 (0x2237) VCh: 17 RFCh: 17 KEEN-CD LAS VEGAS, NV
Channel Number: 17.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 20
Descriptor: ATSC Extended Channel Name Descriptor
Extended Channel Name: BIZ-TV
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language =

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 1.0k | 0
CAT | 0 | 0
PMT | 6 | 0
ETT | 104 | 0
PSIP | 571 | 0
EIT | 398 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,646 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 17 (491 MHz)
Signal: Locked Signal 100 Quality 86
Network Type: ATSC
Run Time: 000:00:51

### PID Usage Chart

0x0000 (0.16% ~ 0.03 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.04% ~ 0.01 Mbps) |  | 0x0030 MPEG-2 PMT for program 17.1/3
0x0031 (55.00% - 10.67 Mbps) |  | 0x0031 MPEG-2 Video for program 17.1/3
0x0034 (1.03% ~ 0.20 Mbps) |  | 0x0034 AC-3 Audio for program 17.1/3
0x0050 (0.04% ~ 0.01 Mbps) |  | 0x0050 MPEG-2 PMT for program 17.3/5
0x0051 (20.86% - 4.04 Mbps) |  | 0x0051 MPEG-2 Video for program 17.3/5
0x0054 (1.03% ~ 0.20 Mbps) |  | 0x0054 AC-3 Audio for program 17.3/5
0x0070 (0.04% ~ 0.01 Mbps) |  | 0x0070 MPEG-2 PMT for program 17.5/7
0x0071 (18.76% - 3.64 Mbps) |  | 0x0071 MPEG-2 Video for program 17.5/7
0x0074 (1.03% ~ 0.20 Mbps) |  | 0x0074 AC-3 Audio for program 17.5/7
0x1d68 (0.11% ~ 0.02 Mbps) |  | 0x1d68 ATSC EIT-0
0x1d69 (0.02% ~ 0.00 Mbps) |  | 0x1d69 ATSC EIT-1
0x1d6a (0.00% ~ 0.00 Mbps) |  | 0x1d6a ATSC EIT-2
0x1d6b (0.00% ~ 0.00 Mbps) |  | 0x1d6b ATSC EIT-3
0x1d6c (0.00% ~ 0.00 Mbps) |  | 0x1d6c ATSC EIT-4
0x1d6d (0.00% ~ 0.00 Mbps) |  | 0x1d6d ATSC EIT-5
0x1d6e (0.00% ~ 0.00 Mbps) |  | 0x1d6e ATSC EIT-6
0x1d6f (0.00% ~ 0.00 Mbps) |  | 0x1d6f ATSC EIT-7
0x1d70 (0.00% ~ 0.00 Mbps) |  | 0x1d70 ATSC EIT-8
0x1d71 (0.00% ~ 0.00 Mbps) |  | 0x1d71 ATSC EIT-9
0x1d72 (0.00% ~ 0.00 Mbps) |  | 0x1d72 ATSC EIT-10
0x1d73 (0.00% ~ 0.00 Mbps) |  | 0x1d73 ATSC EIT-11
0x1d74 (0.00% ~ 0.00 Mbps) |  | 0x1d74 ATSC EIT-12
0x1d75 (0.00% ~ 0.00 Mbps) |  | 0x1d75 ATSC EIT-13
0x1d76 (0.00% ~ 0.00 Mbps) |  | 0x1d76 ATSC EIT-14
0x1d77 (0.00% ~ 0.00 Mbps) |  | 0x1d77 ATSC EIT-15
0x1e68 (0.00% ~ 0.00 Mbps) |  | 0x1e68 ATSC Event ETT-0
0x1e69 (0.00% ~ 0.00 Mbps) |  | 0x1e69 ATSC Event ETT-1
0x1e6a (0.00% ~ 0.00 Mbps) |  | 0x1e6a ATSC Event ETT-2
0x1e6b (0.00% ~ 0.00 Mbps) |  | 0x1e6b ATSC Event ETT-3
0x1e6c (0.00% ~ 0.00 Mbps) |  | 0x1e6c ATSC Event ETT-4
0x1e6d (0.00% ~ 0.00 Mbps) |  | 0x1e6d ATSC Event ETT-5
0x1e6e (0.00% ~ 0.00 Mbps) |  | 0x1e6e ATSC Event ETT-6
0x1e70 (0.00% ~ 0.00 Mbps) |  | 0x1e70 ATSC Event ETT-8
0x1e71 (0.00% ~ 0.00 Mbps) |  | 0x1e71 ATSC Event ETT-9
0x1e72 (0.00% ~ 0.00 Mbps) |  | 0x1e72 ATSC Event ETT-10
0x1e73 (0.00% ~ 0.00 Mbps) |  | 0x1e73 ATSC Event ETT-11
0x1e74 (0.00% ~ 0.00 Mbps) |  | 0x1e74 ATSC Event ETT-12
0x1e75 (0.00% ~ 0.00 Mbps) |  | 0x1e75 ATSC Event ETT-13
0x1e76 (0.00% ~ 0.00 Mbps) |  | 0x1e76 ATSC Event ETT-14
0x1e77 (0.00% ~ 0.00 Mbps) |  | 0x1e77 ATSC Event ETT-15
0x1ffb (0.22% ~ 0.04 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (1.63% ~ 0.32 Mbps) |  | 0x1fff MPEG-2 NULL Packet