### Program Association Table

PAT Version Number: 0
Transport Stream ID: 2411 (0x096b)
PMT PID 1000 (0x03e8) - Program 8.1/1 SOPBSHD
PMT PID 1005 (0x03ed) - Program 8.2/2 PBSWRLD
PMT PID 1010 (0x03f2) - Program 8.3/3 CREATE
PMT PID 1015 (0x03f7) - Program 8.4/4 PBSKIDS

### Program Map Table(s)

Program Number: 8.1/1 SOPBSHD
PCR PID: 0x03e9
Stream Type: 0x02 MPEG-2 Video PID 1001 (0x03e9)
MPEG Video: Bitrate 24.000 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 1002 (0x03ea)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 8.2/2 PBSWRLD
PCR PID: 0x03ee
Stream Type: 0x02 MPEG-2 Video PID 1006 (0x03ee)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Smoothing Buffer Descriptor
Stream Type: 0x81 AC-3 Audio PID 1007 (0x03ef)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 8.3/3 CREATE
PCR PID: 0x03f3
Stream Type: 0x02 MPEG-2 Video PID 1011 (0x03f3)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Smoothing Buffer Descriptor
Stream Type: 0x81 AC-3 Audio PID 1012 (0x03f4)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 8.4/4 PBSKIDS
PCR PID: 0x03f8
Stream Type: 0x02 MPEG-2 Video PID 1016 (0x03f8)
MPEG Video: Bitrate 24.000 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 1017 (0x03f9)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x81 AC-3 Audio PID 1018 (0x03fa)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x81 AC-3 Audio PID 1019 (0x03fb)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: SOPBSHD
TSID: 2411 (0x096b) VCh: 8 RFCh: 8 KSYS MEDFORD, OR
Channel Number: 8.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x03e9
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x03e9 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x03ea Language = eng

Channel 2
Service Name: PBSWRLD
TSID: 2411 (0x096b) VCh: 8 RFCh: 8 KSYS MEDFORD, OR
Channel Number: 8.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x03ee
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x03ee Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x03ef Language = eng

Channel 3
Service Name: CREATE
TSID: 2411 (0x096b) VCh: 8 RFCh: 8 KSYS MEDFORD, OR
Channel Number: 8.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x03f3
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x03f3 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x03f4 Language = eng

Channel 4
Service Name: PBSKIDS
TSID: 2411 (0x096b) VCh: 8 RFCh: 8 KSYS MEDFORD, OR
Channel Number: 8.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x03f8
Stream Type 0x81 (AC-3 Audio) ESPID = 0x03f9 Language = eng
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x03f8 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x03fa Language = spa
Stream Type 0x81 (AC-3 Audio) ESPID = 0x03fb Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 924 | 0
CAT | 0 | 0
PMT | 8 | 0
ETT | 4.1k | 0
PSIP | 665 | 0
EIT | 1.1k | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,678 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 34 (593 MHz)
Signal: Locked Signal 79 Quality 63
Network Type: ATSC
Run Time: 000:00:56

### PID Usage Chart

0x0000 (0.13% ~ 0.03 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x03e8 (0.13% ~ 0.03 Mbps) |  | 0x03e8 MPEG-2 PMT for program 8.1/1
0x03e9 (41.47% - 8.05 Mbps) |  | 0x03e9 MPEG-2 Video for program 8.1/1
0x03ea (1.02% ~ 0.20 Mbps) |  | 0x03ea AC-3 Audio for program 8.1/1
0x03ed (0.13% ~ 0.03 Mbps) |  | 0x03ed MPEG-2 PMT for program 8.2/2
0x03ee (8.65% - 1.68 Mbps) |  | 0x03ee MPEG-2 Video for program 8.2/2
0x03ef (1.02% ~ 0.20 Mbps) |  | 0x03ef AC-3 Audio for program 8.2/2
0x03f2 (0.13% ~ 0.03 Mbps) |  | 0x03f2 MPEG-2 PMT for program 8.3/3
0x03f3 (7.57% - 1.47 Mbps) |  | 0x03f3 MPEG-2 Video for program 8.3/3
0x03f4 (1.02% ~ 0.20 Mbps) |  | 0x03f4 AC-3 Audio for program 8.3/3
0x03f7 (0.13% ~ 0.03 Mbps) |  | 0x03f7 MPEG-2 PMT for program 8.4/4
0x03f8 (32.55% - 6.32 Mbps) |  | 0x03f8 MPEG-2 Video for program 8.4/4
0x03f9 (1.02% ~ 0.20 Mbps) |  | 0x03f9 AC-3 Audio for program 8.4/4
0x03fa (0.68% ~ 0.13 Mbps) |  | 0x03fa AC-3 Audio for program 8.4/4
0x03fb (0.68% ~ 0.13 Mbps) |  | 0x03fb AC-3 Audio for program 8.4/4
0x0911 (0.00% ~ 0.00 Mbps) |  | 0x0911 Unknown usage
0x1d00 (0.17% ~ 0.03 Mbps) |  | 0x1d00 ATSC EIT-0
0x1d01 (0.05% ~ 0.01 Mbps) |  | 0x1d01 ATSC EIT-1
0x1d02 (0.03% ~ 0.01 Mbps) |  | 0x1d02 ATSC EIT-2
0x1d03 (0.02% ~ 0.00 Mbps) |  | 0x1d03 ATSC EIT-3
0x1d04 (0.02% ~ 0.00 Mbps) |  | 0x1d04 ATSC EIT-4
0x1d05 (0.02% ~ 0.00 Mbps) |  | 0x1d05 ATSC EIT-5
0x1d06 (0.01% ~ 0.00 Mbps) |  | 0x1d06 ATSC EIT-6
0x1d07 (0.01% ~ 0.00 Mbps) |  | 0x1d07 ATSC EIT-7
0x1d08 (0.01% ~ 0.00 Mbps) |  | 0x1d08 ATSC EIT-8
0x1d09 (0.01% ~ 0.00 Mbps) |  | 0x1d09 ATSC EIT-9
0x1d0a (0.01% ~ 0.00 Mbps) |  | 0x1d0a ATSC EIT-10
0x1d0b (0.01% ~ 0.00 Mbps) |  | 0x1d0b ATSC EIT-11
0x1d0c (0.01% ~ 0.00 Mbps) |  | 0x1d0c ATSC EIT-12
0x1d0d (0.01% ~ 0.00 Mbps) |  | 0x1d0d ATSC EIT-13
0x1d0e (0.01% ~ 0.00 Mbps) |  | 0x1d0e ATSC EIT-14
0x1d0f (0.00% ~ 0.00 Mbps) |  | 0x1d0f ATSC EIT-15
0x1d10 (0.00% ~ 0.00 Mbps) |  | 0x1d10 ATSC EIT-16
0x1d11 (0.00% ~ 0.00 Mbps) |  | 0x1d11 ATSC EIT-17
0x1d12 (0.00% ~ 0.00 Mbps) |  | 0x1d12 ATSC EIT-18
0x1d13 (0.00% ~ 0.00 Mbps) |  | 0x1d13 ATSC EIT-19
0x1d14 (0.00% ~ 0.00 Mbps) |  | 0x1d14 ATSC EIT-20
0x1d15 (0.00% ~ 0.00 Mbps) |  | 0x1d15 ATSC EIT-21
0x1d16 (0.00% ~ 0.00 Mbps) |  | 0x1d16 ATSC EIT-22
0x1d17 (0.00% ~ 0.00 Mbps) |  | 0x1d17 ATSC EIT-23
0x1e00 (0.27% ~ 0.05 Mbps) |  | 0x1e00 ATSC Event ETT-0
0x1e01 (0.08% ~ 0.02 Mbps) |  | 0x1e01 ATSC Event ETT-1
0x1e02 (0.09% ~ 0.02 Mbps) |  | 0x1e02 ATSC Event ETT-2
0x1e03 (0.05% ~ 0.01 Mbps) |  | 0x1e03 ATSC Event ETT-3
0x1e04 (0.03% ~ 0.01 Mbps) |  | 0x1e04 ATSC Event ETT-4
0x1e05 (0.04% ~ 0.01 Mbps) |  | 0x1e05 ATSC Event ETT-5
0x1e06 (0.04% ~ 0.01 Mbps) |  | 0x1e06 ATSC Event ETT-6
0x1e07 (0.03% ~ 0.00 Mbps) |  | 0x1e07 ATSC Event ETT-7
0x1e08 (0.02% ~ 0.00 Mbps) |  | 0x1e08 ATSC Event ETT-8
0x1e09 (0.02% ~ 0.00 Mbps) |  | 0x1e09 ATSC Event ETT-9
0x1e0a (0.02% ~ 0.00 Mbps) |  | 0x1e0a ATSC Event ETT-10
0x1e0b (0.02% ~ 0.00 Mbps) |  | 0x1e0b ATSC Event ETT-11
0x1e0c (0.02% ~ 0.00 Mbps) |  | 0x1e0c ATSC Event ETT-12
0x1e0d (0.02% ~ 0.00 Mbps) |  | 0x1e0d ATSC Event ETT-13
0x1e0e (0.02% ~ 0.00 Mbps) |  | 0x1e0e ATSC Event ETT-14
0x1e0f (0.01% ~ 0.00 Mbps) |  | 0x1e0f ATSC Event ETT-15
0x1e10 (0.01% ~ 0.00 Mbps) |  | 0x1e10 ATSC Event ETT-16
0x1e11 (0.01% ~ 0.00 Mbps) |  | 0x1e11 ATSC Event ETT-17
0x1e12 (0.01% ~ 0.00 Mbps) |  | 0x1e12 ATSC Event ETT-18
0x1e13 (0.01% ~ 0.00 Mbps) |  | 0x1e13 ATSC Event ETT-19
0x1e14 (0.01% ~ 0.00 Mbps) |  | 0x1e14 ATSC Event ETT-20
0x1e15 (0.01% ~ 0.00 Mbps) |  | 0x1e15 ATSC Event ETT-21
0x1e16 (0.01% ~ 0.00 Mbps) |  | 0x1e16 ATSC Event ETT-22
0x1e17 (0.00% ~ 0.00 Mbps) |  | 0x1e17 ATSC Event ETT-23
0x1ffb (0.30% ~ 0.06 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (2.12% ~ 0.41 Mbps) |  | 0x1fff MPEG-2 NULL Packet