### Program Association Table

PAT Version Number: 1
Transport Stream ID: 1 (0x0001)
PMT PID 48 (0x0030) - Program 26.1/3 KGNGHSN
PMT PID 64 (0x0040) - Program 26.2/4 Tel-Ant
PMT PID 80 (0x0050) - Program 26.3/5 LVT-TV
PMT PID 96 (0x0060) - Program 26.4/6 BUZZR
PMT PID 112 (0x0070) - Program 26.6/7 Ventana
PMT PID 128 (0x0080) - Program 26.8/8 VegasTV
PMT PID 144 (0x0090) - Program 26.9/9 VNA-TV
PMT PID 160 (0x00a0) - Program 26.10/10 QVC2
PMT PID 53 (0x0035) - Program 26.5/11 FLMTV
PMT PID 192 (0x00c0) - Program 26.7/12 MiTele
PMT PID 208 (0x00d0) - Program 26.11/22 BiNGE
PMT PID 224 (0x00e0) - Program 26.12/24 Sales
PMT PID 240 (0x00f0) - Program 26.13/26 Bridge2

### Program Map Table(s)

Program Number: 26.1/3 KGNGHSN
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.2/4 Tel-Ant
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.3/5 LVT-TV
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.4/6 BUZZR
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.6/7 Ventana
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.8/8 VegasTV
PCR PID: 0x0081
Stream Type: 0x02 MPEG-2 Video PID 129 (0x0081)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 132 (0x0084)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.9/9 VNA-TV
PCR PID: 0x0091
Stream Type: 0x02 MPEG-2 Video PID 145 (0x0091)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 148 (0x0094)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.10/10 QVC2
PCR PID: 0x00a1
Stream Type: 0x02 MPEG-2 Video PID 161 (0x00a1)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 164 (0x00a4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.5/11 FLMTV
PCR PID: 0x0037
Stream Type: 0x02 MPEG-2 Video PID 55 (0x0037)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 56 (0x0038)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.7/12 MiTele
PCR PID: 0x00c1
Stream Type: 0x02 MPEG-2 Video PID 193 (0x00c1)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 196 (0x00c4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.11/22 BiNGE
PCR PID: 0x00d1
Stream Type: 0x1b H.264 Video PID 209 (0x00d1)
H.264 Video: Resolution 720 x 480 Interlaced: 1
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 212 (0x00d4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 26.12/24 Sales
PCR PID: 0x0000

Program Number: 26.13/26 Bridge2
PCR PID: 0x00f1
Stream Type: 0x1b H.264 Video PID 241 (0x00f1)
H.264 Video: Resolution 720 x 480 Interlaced: 1
H.264 Video: Framerate: 29.97 Aspect Ratio: Extended SAR
H.264 Profile: High
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 244 (0x00f4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

### Terrestrial Virtual Channel Table

Channel 3
Service Name: KGNGHSN
TSID: 1 (0x0001)
Channel Number: 26.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng

Channel 4
Service Name: Tel-Ant
TSID: 1 (0x0001)
Channel Number: 26.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 5
Service Name: LVT-TV
TSID: 1 (0x0001)
Channel Number: 26.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 6
Service Name: BUZZR
TSID: 1 (0x0001)
Channel Number: 26.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 7
Service Name: Ventana
TSID: 1 (0x0001)
Channel Number: 26.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng

Channel 8
Service Name: VegasTV
TSID: 1 (0x0001)
Channel Number: 26.8
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0081
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0081 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0084 Language = eng

Channel 9
Service Name: VNA-TV
TSID: 1 (0x0001)
Channel Number: 26.9
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 7
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0091
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0091 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0094 Language = eng

Channel 10
Service Name: QVC2
TSID: 1 (0x0001)
Channel Number: 26.10
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 8
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00a1
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x00a1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00a4 Language = eng

Channel 11
Service Name: FLMTV
TSID: 1 (0x0001)
Channel Number: 26.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 9
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0037
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0037 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0038 Language = eng

Channel 12
Service Name: MiTele
TSID: 1 (0x0001)
Channel Number: 26.7
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 10
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00c1
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x00c1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00c4 Language = eng

Channel 22
Service Name: BiNGE
TSID: 1 (0x0001)
Channel Number: 26.11
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 11
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00d1
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x00d1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00d4 Language = eng

Channel 24
Service Name: Sales
TSID: 1 (0x0001)
Channel Number: 26.12
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 12
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00e1
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x00e1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00e4 Language = eng

Channel 26
Service Name: Bridge2
TSID: 1 (0x0001)
Channel Number: 26.13
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 13
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00f1
Stream Type 0x1b (H.264 Video) ESPID = 0x00f1 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00f4 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 671 | 0
CAT | 0 | 0
PMT | 24 | 0
ETT | 0 | 0
PSIP | 1.4k | 0
EIT | 0 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,395,283 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 26 (545 MHz)
Signal: Locked Signal 100 Quality 55
Network Type: ATSC
Run Time: 000:01:13

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.06% ~ 0.01 Mbps) |  | 0x0030 MPEG-2 PMT for program 26.1/3
0x0031 (6.98% - 1.88 Mbps) |  | 0x0031 MPEG-2 Video for program 26.1/3
0x0034 (0.73% ~ 0.14 Mbps) |  | 0x0034 AC-3 Audio for program 26.1/3
0x0035 (0.06% ~ 0.01 Mbps) |  | 0x0035 MPEG-2 PMT for program 26.5/11
0x0037 (6.96% - 2.15 Mbps) |  | 0x0037 MPEG-2 Video for program 26.5/11
0x0038 (0.73% ~ 0.14 Mbps) |  | 0x0038 AC-3 Audio for program 26.5/11
0x0040 (0.06% ~ 0.01 Mbps) |  | 0x0040 MPEG-2 PMT for program 26.2/4
0x0041 (6.96% - 1.92 Mbps) |  | 0x0041 MPEG-2 Video for program 26.2/4
0x0044 (0.73% ~ 0.14 Mbps) |  | 0x0044 AC-3 Audio for program 26.2/4
0x0050 (0.06% ~ 0.01 Mbps) |  | 0x0050 MPEG-2 PMT for program 26.3/5
0x0051 (6.95% - 2.11 Mbps) |  | 0x0051 MPEG-2 Video for program 26.3/5
0x0054 (0.73% ~ 0.14 Mbps) |  | 0x0054 AC-3 Audio for program 26.3/5
0x0060 (0.06% ~ 0.01 Mbps) |  | 0x0060 MPEG-2 PMT for program 26.4/6
0x0061 (6.93% - 2.26 Mbps) |  | 0x0061 MPEG-2 Video for program 26.4/6
0x0064 (0.73% ~ 0.14 Mbps) |  | 0x0064 AC-3 Audio for program 26.4/6
0x0070 (0.06% ~ 0.01 Mbps) |  | 0x0070 MPEG-2 PMT for program 26.6/7
0x0071 (0.21% - 0.04 Mbps) |  | 0x0071 MPEG-2 Video for program 26.6/7
0x0080 (0.06% ~ 0.01 Mbps) |  | 0x0080 MPEG-2 PMT for program 26.8/8
0x0081 (6.96% - 1.90 Mbps) |  | 0x0081 MPEG-2 Video for program 26.8/8
0x0084 (0.73% ~ 0.14 Mbps) |  | 0x0084 AC-3 Audio for program 26.8/8
0x0090 (0.06% ~ 0.01 Mbps) |  | 0x0090 MPEG-2 PMT for program 26.9/9
0x0091 (6.96% - 2.15 Mbps) |  | 0x0091 MPEG-2 Video for program 26.9/9
0x0094 (0.73% ~ 0.14 Mbps) |  | 0x0094 AC-3 Audio for program 26.9/9
0x00a0 (0.06% ~ 0.01 Mbps) |  | 0x00a0 MPEG-2 PMT for program 26.10/10
0x00a1 (6.96% - 2.33 Mbps) |  | 0x00a1 MPEG-2 Video for program 26.10/10
0x00a4 (0.73% ~ 0.14 Mbps) |  | 0x00a4 AC-3 Audio for program 26.10/10
0x00c0 (0.06% ~ 0.01 Mbps) |  | 0x00c0 MPEG-2 PMT for program 26.7/12
0x00c1 (6.97% - 1.94 Mbps) |  | 0x00c1 MPEG-2 Video for program 26.7/12
0x00c4 (0.73% ~ 0.14 Mbps) |  | 0x00c4 AC-3 Audio for program 26.7/12
0x00d0 (0.06% ~ 0.01 Mbps) |  | 0x00d0 MPEG-2 PMT for program 26.11/22
0x00d1 (4.34% - 2.19 Mbps) |  | 0x00d1 H.264 Video for program 26.11/22
0x00d4 (0.73% ~ 0.14 Mbps) |  | 0x00d4 AC-3 Audio for program 26.11/22
0x00f0 (0.06% ~ 0.01 Mbps) |  | 0x00f0 MPEG-2 PMT for program 26.13/26
0x00f1 (4.33% - 1.99 Mbps) |  | 0x00f1 H.264 Video for program 26.13/26
0x00f4 (0.73% ~ 0.14 Mbps) |  | 0x00f4 AC-3 Audio for program 26.13/26
0x1ffb (0.21% ~ 0.04 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (19.45% ~ 3.77 Mbps) |  | 0x1fff MPEG-2 NULL Packet