### Program Association Table

PAT Version Number: 1
Transport Stream ID: 0 (0x0000)
PMT PID 48 (0x0030) - Program 18.1/1 theDove
PMT PID 64 (0x0040) - Program 18.2/2 NewsMax
PMT PID 80 (0x0050) - Program 18.3/3 CBNnews
PMT PID 96 (0x0060) - Program 18.4/4 NRB-TV

### Program Map Table(s)

Program Number: 18.1/1 theDove
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 38.000 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 18.2/2 NewsMax
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 38.000 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 18.3/3 CBNnews
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

Program Number: 18.4/4 NRB-TV
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: theDove
TSID: 0 (0x0000)
Channel Number: 18.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng

Channel 2
Service Name: NewsMax
TSID: 0 (0x0000)
Channel Number: 18.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 3
Service Name: CBNnews
TSID: 0 (0x0000)
Channel Number: 18.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 4
Service Name: NRB-TV
TSID: 0 (0x0000)
Channel Number: 18.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 585 | 0
CAT | 0 | 0
PMT | 8 | 0
ETT | 0 | 0
PSIP | 583 | 0
EIT | 0 | 0

Continuity errors: 13
TEI errors: 72
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,909 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 18 (497 MHz)
Signal: Locked Signal 80 Quality 65
Network Type: ATSC
Run Time: 000:00:53

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x002c (0.00% ~ 0.00 Mbps) *0/1 |  | 0x002c Unknown usage
0x0030 (0.09% ~ 0.02 Mbps) *2/2 |  | 0x0030 MPEG-2 PMT for program 18.1/1
0x0031 (35.28% - 7.38 Mbps) *6/11 |  | 0x0031 MPEG-2 Video for program 18.1/1
0x0032 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0032 Unknown usage
0x0034 (0.73% ~ 0.14 Mbps) *1/0 |  | 0x0034 AC-3 Audio for program 18.1/1
0x0035 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0035 Unknown usage
0x0040 (0.09% ~ 0.02 Mbps) |  | 0x0040 MPEG-2 PMT for program 18.2/2
0x0041 (36.92% - 8.01 Mbps) |  | 0x0041 MPEG-2 Video for program 18.2/2
0x0044 (0.73% ~ 0.14 Mbps) *0/1 |  | 0x0044 AC-3 Audio for program 18.2/2
0x004d (0.00% ~ 0.00 Mbps) *0/1 |  | 0x004d Unknown usage
0x0050 (0.09% ~ 0.02 Mbps) |  | 0x0050 MPEG-2 PMT for program 18.3/3
0x0051 (8.27% - 2.46 Mbps) *0/4 |  | 0x0051 MPEG-2 Video for program 18.3/3
0x0054 (0.73% ~ 0.14 Mbps) |  | 0x0054 AC-3 Audio for program 18.3/3
0x0060 (0.09% ~ 0.02 Mbps) |  | 0x0060 MPEG-2 PMT for program 18.4/4
0x0061 (10.64% - 3.22 Mbps) *1/10 |  | 0x0061 MPEG-2 Video for program 18.4/4
0x0064 (0.73% ~ 0.14 Mbps) *2/1 |  | 0x0064 AC-3 Audio for program 18.4/4
0x0065 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0065 Unknown usage
0x006f (0.00% ~ 0.00 Mbps) *0/1 |  | 0x006f Unknown usage
0x0070 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0070 Unknown usage
0x0071 (0.00% ~ 0.00 Mbps) *1/2 |  | 0x0071 Unknown usage
0x007f (0.00% ~ 0.00 Mbps) *0/1 |  | 0x007f Unknown usage
0x00b1 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x00b1 Unknown usage
0x00f2 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x00f2 Unknown usage
0x00ff (0.00% ~ 0.00 Mbps) *0/1 |  | 0x00ff Unknown usage
0x0131 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0131 Unknown usage
0x0135 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0135 Unknown usage
0x0165 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0165 Unknown usage
0x0181 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0181 Unknown usage
0x0317 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0317 Unknown usage
0x0349 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0349 Unknown usage
0x0361 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0361 Unknown usage
0x0431 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0431 Unknown usage
0x0460 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0460 Unknown usage
0x0461 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0461 Unknown usage
0x04b1 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x04b1 Unknown usage
0x04df (0.00% ~ 0.00 Mbps) *0/1 |  | 0x04df Unknown usage
0x0721 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0721 Unknown usage
0x0f3c (0.00% ~ 0.00 Mbps) *0/1 |  | 0x0f3c Unknown usage
0x1027 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x1027 Unknown usage
0x1030 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x1030 Unknown usage
0x1031 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x1031 Unknown usage
0x1061 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x1061 Unknown usage
0x106f (0.00% ~ 0.00 Mbps) *0/1 |  | 0x106f Unknown usage
0x10c1 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x10c1 Unknown usage
0x1125 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x1125 Unknown usage
0x1132 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x1132 Unknown usage
0x1219 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x1219 Unknown usage
0x1731 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x1731 Unknown usage
0x1831 (0.00% ~ 0.00 Mbps) *0/2 |  | 0x1831 Unknown usage
0x183e (0.00% ~ 0.00 Mbps) *0/1 |  | 0x183e Unknown usage
0x1960 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x1960 Unknown usage
0x1971 (0.00% ~ 0.00 Mbps) *0/1 |  | 0x1971 Unknown usage
0x1ffb (0.10% ~ 0.02 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (5.44% ~ 1.06 Mbps) *0/1 |  | 0x1fff MPEG-2 NULL Packet