### Program Association Table

PAT Version Number: 1
Transport Stream ID: 2087 (0x0827)
PMT PID 48 (0x0030) - Program 15.1/1 Univisn
PMT PID 64 (0x0040) - Program 15.2/2 LATV
PMT PID 96 (0x0060) - Program 15.4/4 TruCrme
PMT PID 112 (0x0070) - Program 15.5/5 Quest
PMT PID 128 (0x0080) - Program 15.6/6 FM

### Program Map Table(s)

Program Number: 15.1/1 Univisn
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 7.811 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x81 AC-3 Audio PID 53 (0x0035)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 15.2/2 LATV
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 1.938 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 15.4/4 TruCrme
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 1.938 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 15.5/5 Quest
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 1.938 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 15.6/6 FM
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0082
Stream Type: 0x02 MPEG-2 Video PID 130 (0x0082)
MPEG Video: Bitrate 0.470 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 132 (0x0084)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: Univisn
TSID: 2087 (0x0827) VCh: 15 RFCh: 16 KINC LAS VEGAS, NV
Channel Number: 15.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = spa
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0035 Language = mul

Channel 2
Service Name: LATV
TSID: 2087 (0x0827) VCh: 15 RFCh: 16 KINC LAS VEGAS, NV
Channel Number: 15.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = spa

Channel 4
Service Name: TruCrme
TSID: 2087 (0x0827) VCh: 15 RFCh: 16 KINC LAS VEGAS, NV
Channel Number: 15.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 5
Service Name: Quest
TSID: 2087 (0x0827) VCh: 15 RFCh: 16 KINC LAS VEGAS, NV
Channel Number: 15.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng

Channel 6
Service Name: FM
TSID: 2087 (0x0827) VCh: 15 RFCh: 16 KINC LAS VEGAS, NV
Channel Number: 15.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0082
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0082 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0084 Language = spa

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 520 | 0
CAT | 0 | 0
PMT | 10 | 0
ETT | 98 | 0
PSIP | 655 | 0
EIT | 652 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,656 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 16 (485 MHz)
Signal: Locked Signal 100 Quality 49
Network Type: ATSC
Run Time: 000:00:45

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.09% ~ 0.02 Mbps) |  | 0x0030 MPEG-2 PMT for program 15.1/1
0x0031 (41.25% - 8.00 Mbps) |  | 0x0031 MPEG-2 Video for program 15.1/1
0x0034 (1.02% ~ 0.20 Mbps) |  | 0x0034 AC-3 Audio for program 15.1/1
0x0035 (1.02% ~ 0.20 Mbps) |  | 0x0035 AC-3 Audio for program 15.1/1
0x0040 (0.09% ~ 0.02 Mbps) |  | 0x0040 MPEG-2 PMT for program 15.2/2
0x0041 (10.31% - 2.00 Mbps) |  | 0x0041 MPEG-2 Video for program 15.2/2
0x0044 (1.02% ~ 0.20 Mbps) |  | 0x0044 AC-3 Audio for program 15.2/2
0x0060 (0.09% ~ 0.02 Mbps) |  | 0x0060 MPEG-2 PMT for program 15.4/4
0x0061 (10.31% - 2.00 Mbps) |  | 0x0061 MPEG-2 Video for program 15.4/4
0x0064 (1.02% ~ 0.20 Mbps) |  | 0x0064 AC-3 Audio for program 15.4/4
0x0070 (0.09% ~ 0.02 Mbps) |  | 0x0070 MPEG-2 PMT for program 15.5/5
0x0071 (10.31% - 2.00 Mbps) |  | 0x0071 MPEG-2 Video for program 15.5/5
0x0074 (1.02% ~ 0.20 Mbps) |  | 0x0074 AC-3 Audio for program 15.5/5
0x0080 (0.09% ~ 0.02 Mbps) |  | 0x0080 MPEG-2 PMT for program 15.6/6
0x0082 (2.79% - 0.54 Mbps) |  | 0x0082 MPEG-2 Video for program 15.6/6
0x0084 (1.23% - 0.24 Mbps) |  | 0x0084 AC-3 Audio for program 15.6/6
0x1388 (0.13% ~ 0.03 Mbps) |  | 0x1388 ATSC EIT-0
0x1389 (0.02% ~ 0.00 Mbps) |  | 0x1389 ATSC EIT-1
0x138a (0.00% ~ 0.00 Mbps) |  | 0x138a ATSC EIT-2
0x138b (0.00% ~ 0.00 Mbps) |  | 0x138b ATSC EIT-3
0x1408 (0.01% ~ 0.00 Mbps) |  | 0x1408 ATSC Event ETT-0
0x1409 (0.00% ~ 0.00 Mbps) |  | 0x1409 ATSC Event ETT-1
0x140a (0.00% ~ 0.00 Mbps) |  | 0x140a ATSC Event ETT-2
0x140b (0.00% ~ 0.00 Mbps) |  | 0x140b ATSC Event ETT-3
0x1ffb (0.14% ~ 0.03 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (17.84% ~ 3.46 Mbps) |  | 0x1fff MPEG-2 NULL Packet