### Program Association Table

PAT Version Number: 8
Transport Stream ID: 2 (0x0002)
PMT PID 64 (0x0040) - Program 18.2/4 FUN
PMT PID 80 (0x0050) - Program 18.3/5 RNTV
PMT PID 96 (0x0060) - Program 18.5/6 ACE
PMT PID 112 (0x0070) - Program 18.4/7 BARK
PMT PID 128 (0x0080) - Program 18.6/8 VEN
PMT PID 160 (0x00a0) - Program 18.7/10 RVTV
PMT PID 176 (0x00b0) - Program 18.8/11 MOT
PMT PID 176 (0x00b0) - Program 18.9/12 Blues

### Program Map Table(s)

Program Number: 18.2/4 FUN
Descriptor: Registration Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 4.716 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 18.3/5 RNTV
Descriptor: Registration Descriptor
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 4.716 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 18.5/6 ACE
Descriptor: Registration Descriptor
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 4.716 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 18.4/7 BARK
Descriptor: Registration Descriptor
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 4.716 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 18.6/8 VEN
Descriptor: Registration Descriptor
PCR PID: 0x0081
Stream Type: 0x02 MPEG-2 Video PID 129 (0x0081)
MPEG Video: Bitrate 4.716 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 132 (0x0084)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 18.7/10 RVTV
Descriptor: Registration Descriptor
PCR PID: 0x00a1
Stream Type: 0x02 MPEG-2 Video PID 161 (0x00a1)
MPEG Video: Bitrate 4.716 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 164 (0x00a4)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 18.8/11 MOT
Descriptor: Registration Descriptor
PCR PID: 0x00b1
Stream Type: 0x02 MPEG-2 Video PID 177 (0x00b1)
MPEG Video: Bitrate 4.716 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 180 (0x00b4)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 18.9/12 Blues
Descriptor: Registration Descriptor
PCR PID: 0x03e8
Stream Type: 0x02 MPEG-2 Video PID 1000 (0x03e8)
MPEG Video: Bitrate 4.716 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 1001 (0x03e9)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 4
Service Name: FUN
TSID: 2 (0x0002)
Channel Number: 18.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 5
Service Name: RNTV
TSID: 2 (0x0002)
Channel Number: 18.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 6
Service Name: ACE
TSID: 2 (0x0002)
Channel Number: 18.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 7
Service Name: BARK
TSID: 2 (0x0002)
Channel Number: 18.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 7
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng

Channel 8
Service Name: VEN
TSID: 2 (0x0002)
Channel Number: 18.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 8
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0081
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0081 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0084 Language = eng

Channel 10
Service Name: RVTV
TSID: 2 (0x0002)
Channel Number: 18.7
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 10
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00a1
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x00a1 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00a4 Language = eng

Channel 11
Service Name: MOT
TSID: 2 (0x0002)
Channel Number: 18.8
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 11
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00b1
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x00b1 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00b4 Language = eng

Channel 12
Service Name: Blues
TSID: 2 (0x0002)
Channel Number: 18.9
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 11
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x03e8
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x03e8 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x03e9 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 1.5k | 0
CAT | 0 | 0
PMT | 15 | 0
ETT | 0 | 0
PSIP | 1.7k | 0
EIT | 0 | 0

Continuity errors: 21
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,393,247 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 27 (551 MHz)
Signal: Locked Signal 90 Quality 67
Network Type: ATSC
Run Time: 000:02:21

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0040 (0.02% ~ 0.00 Mbps) |  | 0x0040 MPEG-2 PMT for program 18.2/4
0x0041 (11.62% - 2.26 Mbps) *3/0 |  | 0x0041 MPEG-2 Video for program 18.2/4
0x0044 (1.02% ~ 0.20 Mbps) |  | 0x0044 AC-3 Audio for program 18.2/4
0x0050 (0.02% ~ 0.00 Mbps) |  | 0x0050 MPEG-2 PMT for program 18.3/5
0x0051 (14.49% - 2.81 Mbps) *4/0 |  | 0x0051 MPEG-2 Video for program 18.3/5
0x0054 (1.02% ~ 0.20 Mbps) |  | 0x0054 AC-3 Audio for program 18.3/5
0x0060 (0.02% ~ 0.00 Mbps) |  | 0x0060 MPEG-2 PMT for program 18.5/6
0x0061 (8.36% - 1.63 Mbps) *2/0 |  | 0x0061 MPEG-2 Video for program 18.5/6
0x0064 (1.02% ~ 0.20 Mbps) |  | 0x0064 AC-3 Audio for program 18.5/6
0x0070 (0.02% ~ 0.00 Mbps) |  | 0x0070 MPEG-2 PMT for program 18.4/7
0x0071 (15.09% - 2.93 Mbps) *4/0 |  | 0x0071 MPEG-2 Video for program 18.4/7
0x0074 (1.02% ~ 0.20 Mbps) |  | 0x0074 AC-3 Audio for program 18.4/7
0x0080 (0.02% ~ 0.00 Mbps) |  | 0x0080 MPEG-2 PMT for program 18.6/8
0x0081 (7.43% - 1.44 Mbps) |  | 0x0081 MPEG-2 Video for program 18.6/8
0x0084 (1.02% ~ 0.20 Mbps) |  | 0x0084 AC-3 Audio for program 18.6/8
0x00a0 (0.02% ~ 0.00 Mbps) |  | 0x00a0 MPEG-2 PMT for program 18.7/10
0x00a1 (12.40% - 2.41 Mbps) *3/0 |  | 0x00a1 MPEG-2 Video for program 18.7/10
0x00a4 (1.02% ~ 0.20 Mbps) *1/0 |  | 0x00a4 AC-3 Audio for program 18.7/10
0x00b0 (0.04% ~ 0.01 Mbps) |  | 0x00b0 MPEG-2 PMT for program 18.8/11
0x00b1 (7.87% - 1.53 Mbps) *2/0 |  | 0x00b1 MPEG-2 Video for program 18.8/11
0x00b4 (1.02% ~ 0.20 Mbps) *1/0 |  | 0x00b4 AC-3 Audio for program 18.8/11
0x03e8 (13.71% - 2.66 Mbps) *1/0 |  | 0x03e8 MPEG-2 Video for program 18.9/12
0x03e9 (1.02% ~ 0.20 Mbps) |  | 0x03e9 AC-3 Audio for program 18.9/12
0x1ffb (0.15% ~ 0.03 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (0.49% ~ 0.09 Mbps) |  | 0x1fff MPEG-2 NULL Packet