### Program Association Table

PAT Version Number: 1
Transport Stream ID: 9545 (0x2549)
PMT PID 48 (0x0030) - Program 27.1/1 UniMas
PMT PID 64 (0x0040) - Program 27.88/2 AltaVsn

### Program Map Table(s)

Program Number: 27.1/1 UniMas
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 7.811 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Stream Type: 0x81 AC-3 Audio PID 53 (0x0035)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 27.88/2 AltaVsn
Descriptor: Smoothing Buffer Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 6.627 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 59.94 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: UniMas
TSID: 9545 (0x2549) VCh: 27 RFCh: 15 KELV-LD LAS VEGAS, NV
Channel Number: 27.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = spa
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0035 Language = mul

Channel 2
Service Name: AltaVsn
TSID: 9545 (0x2549) VCh: 27 RFCh: 15 KELV-LD LAS VEGAS, NV
Channel Number: 27.88
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = spa

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 135 | 0
CAT | 0 | 0
PMT | 4 | 0
ETT | 27 | 0
PSIP | 171 | 0
EIT | 69 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,796 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 15 (479 MHz)
Signal: Locked Signal 99 Quality 67
Network Type: ATSC
Run Time: 000:00:12

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.09% ~ 0.02 Mbps) |  | 0x0030 MPEG-2 PMT for program 27.1/1
0x0031 (41.25% - 8.03 Mbps) |  | 0x0031 MPEG-2 Video for program 27.1/1
0x0034 (1.02% ~ 0.20 Mbps) |  | 0x0034 AC-3 Audio for program 27.1/1
0x0035 (1.02% ~ 0.20 Mbps) |  | 0x0035 AC-3 Audio for program 27.1/1
0x0040 (0.09% ~ 0.02 Mbps) |  | 0x0040 MPEG-2 PMT for program 27.88/2
0x0041 (35.06% - 6.80 Mbps) |  | 0x0041 MPEG-2 Video for program 27.88/2
0x0044 (0.68% ~ 0.13 Mbps) |  | 0x0044 AC-3 Audio for program 27.88/2
0x1388 (0.06% ~ 0.01 Mbps) |  | 0x1388 ATSC EIT-0
0x1389 (0.01% ~ 0.00 Mbps) |  | 0x1389 ATSC EIT-1
0x138a (0.00% ~ 0.00 Mbps) |  | 0x138a ATSC EIT-2
0x138b (0.00% ~ 0.00 Mbps) |  | 0x138b ATSC EIT-3
0x1408 (0.01% ~ 0.00 Mbps) |  | 0x1408 ATSC Event ETT-0
0x1409 (0.01% ~ 0.00 Mbps) |  | 0x1409 ATSC Event ETT-1
0x140a (0.00% ~ 0.00 Mbps) |  | 0x140a ATSC Event ETT-2
0x140b (0.00% ~ 0.00 Mbps) |  | 0x140b ATSC Event ETT-3
0x1ffb (0.11% ~ 0.02 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (20.48% ~ 3.97 Mbps) |  | 0x1fff MPEG-2 NULL Packet