### Program Association Table

PAT Version Number: 2
Transport Stream ID: 9825 (0x2661)
PMT PID 48 (0x0030) - Program 24.1/1 theDove
PMT PID 64 (0x0040) - Program 24.2/2 NewsMax
PMT PID 80 (0x0050) - Program 24.3/3 CBNnews
PMT PID 96 (0x0060) - Program 24.4/4 NRB-TV

### Program Map Table(s)

Program Number: 24.1/1 theDove
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 38.000 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 24.2/2 NewsMax
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 38.000 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 24.3/3 CBNnews
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R

Program Number: 24.4/4 NRB-TV
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 15.000 Mbps Resolution 720 x 480p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: STD Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Data Stream Alignment Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: ATSC AC-3 audio Descriptor
Descriptor: ISO639 Language Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: theDove
TSID: 9825 (0x2661) VCh: 43 RFCh: 16 KDSO-LD MEDFORD, OR
Channel Number: 24.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng

Channel 2
Service Name: NewsMax
TSID: 9825 (0x2661) VCh: 43 RFCh: 16 KDSO-LD MEDFORD, OR
Channel Number: 24.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 3
Service Name: CBNnews
TSID: 9825 (0x2661) VCh: 43 RFCh: 16 KDSO-LD MEDFORD, OR
Channel Number: 24.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 4
Service Name: NRB-TV
TSID: 9825 (0x2661) VCh: 43 RFCh: 16 KDSO-LD MEDFORD, OR
Channel Number: 24.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language = eng
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 579 | 0
CAT | 0 | 0
PMT | 8 | 0
ETT | 0 | 0
PSIP | 577 | 0
EIT | 0 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,102 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 24 (533 MHz)
Signal: Locked Signal 78 Quality 71
Network Type: ATSC
Run Time: 000:00:53

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.09% ~ 0.02 Mbps) |  | 0x0030 MPEG-2 PMT for program 24.1/1
0x0031 (33.06% - 7.08 Mbps) |  | 0x0031 MPEG-2 Video for program 24.1/1
0x0034 (0.73% ~ 0.14 Mbps) |  | 0x0034 AC-3 Audio for program 24.1/1
0x0040 (0.09% ~ 0.02 Mbps) |  | 0x0040 MPEG-2 PMT for program 24.2/2
0x0041 (35.38% - 7.75 Mbps) |  | 0x0041 MPEG-2 Video for program 24.2/2
0x0044 (0.73% ~ 0.14 Mbps) |  | 0x0044 AC-3 Audio for program 24.2/2
0x0050 (0.09% ~ 0.02 Mbps) |  | 0x0050 MPEG-2 PMT for program 24.3/3
0x0051 (13.58% - 3.74 Mbps) |  | 0x0051 MPEG-2 Video for program 24.3/3
0x0054 (0.73% ~ 0.14 Mbps) |  | 0x0054 AC-3 Audio for program 24.3/3
0x0060 (0.09% ~ 0.02 Mbps) |  | 0x0060 MPEG-2 PMT for program 24.4/4
0x0061 (9.24% - 2.86 Mbps) |  | 0x0061 MPEG-2 Video for program 24.4/4
0x0064 (0.73% ~ 0.14 Mbps) |  | 0x0064 AC-3 Audio for program 24.4/4
0x1ffb (0.11% ~ 0.02 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (5.29% ~ 1.03 Mbps) |  | 0x1fff MPEG-2 NULL Packet