### Program Association Table

PAT Version Number: 13
Transport Stream ID: 6067 (0x17b3)
PMT PID 48 (0x0030) - Program 25.1/3 PrimeHD
PMT PID 64 (0x0040) - Program 25.2/4 Movies!
PMT PID 80 (0x0050) - Program 25.3/5 RAV HD
PMT PID 96 (0x0060) - Program 25.4/6 OAN
PMT PID 112 (0x0070) - Program 25.5/7 NEWSMAX
PMT PID 128 (0x0080) - Program 25.6/8 Story
PMT PID 144 (0x0090) - Program 25.7/9 AWE MP4
PMT PID 160 (0x00a0) - Program 25.8/10 KACEMP4
PMT PID 176 (0x00b0) - Program 25.9/11 Lease
PMT PID 192 (0x00c0) - Program 25.10/12 Uncion

### Program Map Table(s)

Program Number: 25.1/3 PrimeHD
Descriptor: Registration Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 19.674 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 25.2/4 Movies!
Descriptor: Registration Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 19.740 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 25.3/5 RAV HD
Descriptor: Registration Descriptor
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 19.740 Mbps Resolution 1280 x 720p
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 25.4/6 OAN
Descriptor: Registration Descriptor
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 19.740 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 25.5/7 NEWSMAX
Descriptor: Registration Descriptor
PCR PID: 0x0071
Stream Type: 0x02 MPEG-2 Video PID 113 (0x0071)
MPEG Video: Bitrate 19.740 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 116 (0x0074)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 25.6/8 Story
Descriptor: Registration Descriptor
PCR PID: 0x0081
Stream Type: 0x02 MPEG-2 Video PID 129 (0x0081)
MPEG Video: Bitrate 19.740 Mbps Resolution 720 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Stream Type: 0x81 AC-3 Audio PID 132 (0x0084)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 25.7/9 AWE MP4
Descriptor: Registration Descriptor
PCR PID: 0x0091
Stream Type: 0x1b H.264 Video PID 145 (0x0091)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: 40:33
H.264 Profile: High
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: AVC video Descriptor
Stream Type: 0x81 AC-3 Audio PID 148 (0x0094)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 25.8/10 KACEMP4
Descriptor: Registration Descriptor
PCR PID: 0x00a1
Stream Type: 0x1b H.264 Video PID 161 (0x00a1)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: 40:33
H.264 Profile: High
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: AVC video Descriptor
Stream Type: 0x81 AC-3 Audio PID 164 (0x00a4)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 25.9/11 Lease
Descriptor: Registration Descriptor
PCR PID: 0x00b1
Stream Type: 0x1b H.264 Video PID 177 (0x00b1)
H.264 Video: Resolution 720 x 480 Interlaced: 1
H.264 Video: Framerate: 29.97 Aspect Ratio: 1:1 (square)
H.264 Profile: High
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: AVC video Descriptor
Stream Type: 0x81 AC-3 Audio PID 180 (0x00b4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 25.10/12 Uncion
Descriptor: Registration Descriptor
PCR PID: 0x00c1
Stream Type: 0x1b H.264 Video PID 193 (0x00c1)
H.264 Video: Resolution 720 x 480 Interlaced: 0
H.264 Video: Framerate: 29.97 Aspect Ratio: 40:33
H.264 Profile: High
Descriptor: Data Stream Alignment Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: AVC video Descriptor
Stream Type: 0x81 AC-3 Audio PID 196 (0x00c4)
AC3: Bitrate 128 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: Registration Descriptor
Descriptor: ISO639 Language Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 3
Service Name: PrimeHD
TSID: 6067 (0x17b3) VCh: 46 RFCh: 25 KPVM-LD PAHRUMP, NV
Channel Number: 25.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng

Channel 4
Service Name: Movies!
TSID: 6067 (0x17b3) VCh: 46 RFCh: 25 KPVM-LD PAHRUMP, NV
Channel Number: 25.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng

Channel 5
Service Name: RAV HD
TSID: 6067 (0x17b3) VCh: 46 RFCh: 25 KPVM-LD PAHRUMP, NV
Channel Number: 25.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 5
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng

Channel 6
Service Name: OAN
TSID: 6067 (0x17b3) VCh: 46 RFCh: 25 KPVM-LD PAHRUMP, NV
Channel Number: 25.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 6
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng

Channel 7
Service Name: NEWSMAX
TSID: 6067 (0x17b3) VCh: 46 RFCh: 25 KPVM-LD PAHRUMP, NV
Channel Number: 25.5
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 7
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0071
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0071 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0074 Language = eng

Channel 8
Service Name: Story
TSID: 6067 (0x17b3) VCh: 46 RFCh: 25 KPVM-LD PAHRUMP, NV
Channel Number: 25.6
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 8
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0081
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0081 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0084 Language = eng

Channel 9
Service Name: AWE MP4
TSID: 6067 (0x17b3) VCh: 46 RFCh: 25 KPVM-LD PAHRUMP, NV
Channel Number: 25.7
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 9
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0091
Stream Type 0x1b (H.264 Video) ESPID = 0x0091 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0094 Language = eng

Channel 10
Service Name: KACEMP4
TSID: 6067 (0x17b3) VCh: 46 RFCh: 25 KPVM-LD PAHRUMP, NV
Channel Number: 25.8
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 10
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00a1
Stream Type 0x1b (H.264 Video) ESPID = 0x00a1 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00a4 Language = eng

Channel 11
Service Name: Lease
TSID: 6067 (0x17b3) VCh: 46 RFCh: 25 KPVM-LD PAHRUMP, NV
Channel Number: 25.9
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 11
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00b1
Stream Type 0x1b (H.264 Video) ESPID = 0x00b1 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00b4 Language = eng

Channel 12
Service Name: Uncion
TSID: 6067 (0x17b3) VCh: 46 RFCh: 25 KPVM-LD PAHRUMP, NV
Channel Number: 25.10
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 12
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x00c1
Stream Type 0x1b (H.264 Video) ESPID = 0x00c1 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x00c4 Language = spa

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 480 | 0
CAT | 0 | 0
PMT | 20 | 0
ETT | 661 | 0
PSIP | 580 | 0
EIT | 169 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,584 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 25 (539 MHz)
Signal: Locked Signal 100 Quality 75
Network Type: ATSC
Run Time: 000:00:48

### PID Usage Chart

0x0000 (0.09% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.02% ~ 0.00 Mbps) |  | 0x0030 MPEG-2 PMT for program 25.1/3
0x0031 (20.71% - 4.02 Mbps) |  | 0x0031 MPEG-2 Video for program 25.1/3
0x0034 (1.02% ~ 0.20 Mbps) |  | 0x0034 AC-3 Audio for program 25.1/3
0x0040 (0.02% ~ 0.00 Mbps) |  | 0x0040 MPEG-2 PMT for program 25.2/4
0x0041 (7.82% - 1.52 Mbps) |  | 0x0041 MPEG-2 Video for program 25.2/4
0x0044 (0.68% ~ 0.13 Mbps) |  | 0x0044 AC-3 Audio for program 25.2/4
0x0050 (0.02% ~ 0.00 Mbps) |  | 0x0050 MPEG-2 PMT for program 25.3/5
0x0051 (23.28% - 4.52 Mbps) |  | 0x0051 MPEG-2 Video for program 25.3/5
0x0054 (0.68% ~ 0.13 Mbps) |  | 0x0054 AC-3 Audio for program 25.3/5
0x0060 (0.02% ~ 0.00 Mbps) |  | 0x0060 MPEG-2 PMT for program 25.4/6
0x0061 (9.32% - 1.81 Mbps) |  | 0x0061 MPEG-2 Video for program 25.4/6
0x0064 (0.68% ~ 0.13 Mbps) |  | 0x0064 AC-3 Audio for program 25.4/6
0x0070 (0.02% ~ 0.00 Mbps) |  | 0x0070 MPEG-2 PMT for program 25.5/7
0x0071 (8.64% - 1.67 Mbps) |  | 0x0071 MPEG-2 Video for program 25.5/7
0x0074 (0.68% ~ 0.13 Mbps) |  | 0x0074 AC-3 Audio for program 25.5/7
0x0080 (0.02% ~ 0.00 Mbps) |  | 0x0080 MPEG-2 PMT for program 25.6/8
0x0081 (7.59% - 1.47 Mbps) |  | 0x0081 MPEG-2 Video for program 25.6/8
0x0084 (0.68% ~ 0.13 Mbps) |  | 0x0084 AC-3 Audio for program 25.6/8
0x0090 (0.02% ~ 0.00 Mbps) |  | 0x0090 MPEG-2 PMT for program 25.7/9
0x0091 (5.99% - 1.16 Mbps) |  | 0x0091 H.264 Video for program 25.7/9
0x0094 (0.68% ~ 0.13 Mbps) |  | 0x0094 AC-3 Audio for program 25.7/9
0x00a0 (0.02% ~ 0.00 Mbps) |  | 0x00a0 MPEG-2 PMT for program 25.8/10
0x00a1 (2.12% - 0.41 Mbps) |  | 0x00a1 H.264 Video for program 25.8/10
0x00a4 (1.02% ~ 0.20 Mbps) |  | 0x00a4 AC-3 Audio for program 25.8/10
0x00b0 (0.02% ~ 0.00 Mbps) |  | 0x00b0 MPEG-2 PMT for program 25.9/11
0x00b1 (2.08% - 0.40 Mbps) |  | 0x00b1 H.264 Video for program 25.9/11
0x00b4 (0.68% ~ 0.13 Mbps) |  | 0x00b4 AC-3 Audio for program 25.9/11
0x00c0 (0.02% ~ 0.00 Mbps) |  | 0x00c0 MPEG-2 PMT for program 25.10/12
0x00c1 (3.86% - 0.75 Mbps) |  | 0x00c1 H.264 Video for program 25.10/12
0x00c4 (0.68% ~ 0.13 Mbps) |  | 0x00c4 AC-3 Audio for program 25.10/12
0x0fa0 (0.04% ~ 0.01 Mbps) |  | 0x0fa0 ATSC EIT-0
0x0fa1 (0.01% ~ 0.00 Mbps) |  | 0x0fa1 ATSC EIT-1
0x0fa2 (0.00% ~ 0.00 Mbps) |  | 0x0fa2 ATSC EIT-2
0x0fa3 (0.00% ~ 0.00 Mbps) |  | 0x0fa3 ATSC EIT-3
0x0fa4 (0.00% ~ 0.00 Mbps) |  | 0x0fa4 ATSC EIT-4
0x1388 (0.07% ~ 0.01 Mbps) |  | 0x1388 ATSC Event ETT-0
0x1389 (0.02% ~ 0.00 Mbps) |  | 0x1389 ATSC Event ETT-1
0x138a (0.01% ~ 0.00 Mbps) |  | 0x138a ATSC Event ETT-2
0x138b (0.01% ~ 0.00 Mbps) |  | 0x138b ATSC Event ETT-3
0x138c (0.01% ~ 0.00 Mbps) |  | 0x138c ATSC Event ETT-4
0x1ffb (0.15% ~ 0.03 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (0.52% ~ 0.10 Mbps) |  | 0x1fff MPEG-2 NULL Packet