### Program Association Table

PAT Version Number: 0
Transport Stream ID: 2827 (0x0b0b)
PMT PID 48 (0x0030) - Program 30.1/1 KBLN-DT
PMT PID 64 (0x0040) - Program 30.2/2 BLBN-2
PMT PID 80 (0x0050) - Program 30.3/3 BLBN-3
PMT PID 96 (0x0060) - Program 30.4/4 BLBN-4

### Program Map Table(s)

Program Number: 30.1/1 KBLN-DT
Descriptor: System Clock Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Registration Descriptor
PCR PID: 0x0031
Stream Type: 0x02 MPEG-2 Video PID 49 (0x0031)
MPEG Video: Bitrate 80.000 Mbps Resolution 1920 x 1080i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Stream Type: 0x81 AC-3 Audio PID 52 (0x0034)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 30.2/2 BLBN-2
Descriptor: System Clock Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Registration Descriptor
PCR PID: 0x0041
Stream Type: 0x02 MPEG-2 Video PID 65 (0x0041)
MPEG Video: Bitrate 3.999 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Stream Type: 0x81 AC-3 Audio PID 68 (0x0044)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 30.3/3 BLBN-3
Descriptor: System Clock Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Registration Descriptor
PCR PID: 0x0051
Stream Type: 0x02 MPEG-2 Video PID 81 (0x0051)
MPEG Video: Bitrate 3.999 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Stream Type: 0x81 AC-3 Audio PID 84 (0x0054)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor

Program Number: 30.4/4 BLBN-4
Descriptor: System Clock Descriptor
Descriptor: Maximum Bitrate Descriptor
Descriptor: Smoothing Buffer Descriptor
Descriptor: Registration Descriptor
PCR PID: 0x0061
Stream Type: 0x02 MPEG-2 Video PID 97 (0x0061)
MPEG Video: Bitrate 3.999 Mbps Resolution 704 x 480i
MPEG Video: Framerate 29.97 fps Aspect Ratio 16:9
MPEG Video: Chroma Format 4:2:0
Descriptor: Video Stream Descriptor
Stream Type: 0x81 AC-3 Audio PID 100 (0x0064)
AC3: Bitrate 192 Kbps Sample Rate 48 KHz
AC3: Mode complete main Coding 2/0 L, R
Descriptor: ISO639 Language Descriptor
Descriptor: Registration Descriptor
Descriptor: ATSC AC-3 audio Descriptor

### Terrestrial Virtual Channel Table

Channel 1
Service Name: KBLN-DT
TSID: 2827 (0x0b0b) VCh: 13 RFCh: 13 KCOS EL PASO, TX
Channel Number: 30.1
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 1
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0031
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0031 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0034 Language = eng
Descriptor: ATSC Extended Channel Name Descriptor
Extended Channel Name: KBLN-DT

Channel 2
Service Name: BLBN-2
TSID: 2827 (0x0b0b) VCh: 13 RFCh: 13 KCOS EL PASO, TX
Channel Number: 30.2
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 2
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0041
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0041 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0044 Language = eng
Descriptor: ATSC Extended Channel Name Descriptor
Extended Channel Name: BLBN-2

Channel 3
Service Name: BLBN-3
TSID: 2827 (0x0b0b) VCh: 13 RFCh: 13 KCOS EL PASO, TX
Channel Number: 30.3
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 3
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0051
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0051 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0054 Language = eng
Descriptor: ATSC Extended Channel Name Descriptor
Extended Channel Name: BLBN-3

Channel 4
Service Name: BLBN-4
TSID: 2827 (0x0b0b) VCh: 13 RFCh: 13 KCOS EL PASO, TX
Channel Number: 30.4
Carrier Frequency: 0
Modulation Mode: ATSC (8 VSB)
Source ID: 4
Descriptor: ATSC Service Location Descriptor
Service Location Descriptor:
PCR PID 0x0061
Stream Type 0x02 (MPEG-2 Video) ESPID = 0x0061 Language =
Stream Type 0x81 (AC-3 Audio) ESPID = 0x0064 Language = eng
Descriptor: ATSC Extended Channel Name Descriptor
Extended Channel Name: BLBN-4

### MPEG-2 Statistics

Table | Sections Processed | CRC Errors
PAT | 441 | 0
CAT | 0 | 0
PMT | 8 | 0
ETT | 0 | 0
PSIP | 447 | 0
EIT | 532 | 0

Continuity errors: 0
TEI errors: 0
Sync Losses: 0
Retunes: 0
Calculated multiplex rate: 19,392,836 bps

### General Information

Source: HDHomeRun 8VSB (ATSC)
Tuner: Channel 23 (527 MHz)
Signal: Locked Signal 77 Quality 69
Network Type: ATSC
Run Time: 000:00:43

### PID Usage Chart

0x0000 (0.08% ~ 0.02 Mbps) |  | 0x0000 MPEG-2 Program Assocation Table
0x0030 (0.02% ~ 0.00 Mbps) |  | 0x0030 MPEG-2 PMT for program 30.1/1
0x0031 (30.94% - 6.00 Mbps) |  | 0x0031 MPEG-2 Video for program 30.1/1
0x0034 (1.02% ~ 0.20 Mbps) |  | 0x0034 AC-3 Audio for program 30.1/1
0x0040 (0.02% ~ 0.00 Mbps) |  | 0x0040 MPEG-2 PMT for program 30.2/2
0x0041 (20.62% - 4.00 Mbps) |  | 0x0041 MPEG-2 Video for program 30.2/2
0x0044 (1.02% ~ 0.20 Mbps) |  | 0x0044 AC-3 Audio for program 30.2/2
0x0050 (0.02% ~ 0.00 Mbps) |  | 0x0050 MPEG-2 PMT for program 30.3/3
0x0051 (20.62% - 4.00 Mbps) |  | 0x0051 MPEG-2 Video for program 30.3/3
0x0054 (1.02% ~ 0.20 Mbps) |  | 0x0054 AC-3 Audio for program 30.3/3
0x0060 (0.02% ~ 0.00 Mbps) |  | 0x0060 MPEG-2 PMT for program 30.4/4
0x0061 (20.62% - 4.00 Mbps) |  | 0x0061 MPEG-2 Video for program 30.4/4
0x0064 (1.02% ~ 0.20 Mbps) |  | 0x0064 AC-3 Audio for program 30.4/4
0x1fd0 (0.07% ~ 0.01 Mbps) |  | 0x1fd0 ATSC EIT-0
0x1fd1 (0.01% ~ 0.00 Mbps) |  | 0x1fd1 ATSC EIT-1
0x1fd2 (0.01% ~ 0.00 Mbps) |  | 0x1fd2 ATSC EIT-2
0x1fd3 (0.01% ~ 0.00 Mbps) |  | 0x1fd3 ATSC EIT-3
0x1ffb (0.10% ~ 0.02 Mbps) |  | 0x1ffb ATSC Base PID (TVCT, MGT, RT, STT)
0x1fff (2.76% ~ 0.54 Mbps) |  | 0x1fff MPEG-2 NULL Packet